0 0

1

Bit Serial Reconfigurable Bit Parallel

1 0 0 1

ALU ALU ALU ALU ALU

Memory Bit