Blind Walking of a Planar Biped on Sloped Terrain by

Chee-Meng Chew

B.Eng. Mech. (Hons)

NationalUniversityofSingapore

SUBMITTED TO THE DEPARTMENT OF MECHANICAL ENGINEERING

IN PARTIAL FULFILLMENT OF THE REQUIREMENTS FOR THE DEGREE OF

MASTER OF SCIENCE IN MECHANICAL ENGINEERING

AT THE

MASSACHUSETTS INSTITUTE OF TECHNOLOGY

FEBRUARY 1998

© 1998 Chee-Meng Chew. Allrights reserved.

The author herebygrants to MIT permission to reproduce and to distribute publiclypaper and electronic copies ofthis thesis document in whole or in part.

Signature ofAuthor ................................ ................................ ................................ ..........

Department ofMechanicalEngineering

January16, 1998

Certified by ................................ ................................ ................................ .......................

GillA. Pratt

Assistant Professor, ElectricalEngineering and Computer Science

Thesis Supervisor

Certified by ................................ ................................ ................................ .......................

Jean-Jacques E. Slotine

Professor, MechanicalEngineering

Thesis Reader

Certified by ................................ ................................ ................................ .......................

Ain A. Sonin

Chairman, DepartmentalCommittee on Graduate Students

Blind Walking of a Planar Biped on Sloped Terrain by

Chee-Meng Chew

Submitted to the Department of Mechanical Engineering on January15, 1998 in Partial Fulfillment of the

Requirements for the Degree of Master of Science in

Mechanical Engineering

ABSTRACT

This thesis demonstrates the successful application of Virtual Model Control (VMC) to a simulated sevenlink planar biped for walking dynamically and steadily over sloped terrain with unknown slope gradients and transition locations. The slope gradients were assumed to be between ± 20 o ; and it had maximum transitional gradient change of less than 20 o per step. The developed algorithm for sloped terrain walking was based on a level ground implementation with onlyminor changes. This thesis adopted the same virtual components, which included a vertical spring-damper, a horizontal damper and a rotational spring-damper, to generate the required torque at the joints. The biped used the natural compliance of swing foot so that it could land flat onto an unknown slope. After the complete touch down of the swing foot, a global slope was computed and this was used to define a virtual surface . The algorithm then computed the desired hip height based on the global slope which resulted in a desired straight line trajectoryparallel to the virtual surface. The algorithm was verysimple and did not require the biped to have an extensive sensorysystem for blind walking over slopes. The ground was detected onlythrough foot contact switches. The knowledge required for the implementation mainlyconsisted of intuition and geometric considerations.

This thesis also demonsrates the replacement of the vertical virtual spring-damper with Robust Adaptive

Controller and the successful implementation with the biped walking over random sloped terrain. This thesis also shows howthe algorithm for sloped terrain walking can be extended to stair climbing.

Thesis Supervisor: Gill A. Pratt, Ph.D.

Title: Assistant Professor of Electrical Engineering and Computer Science

Acknow ledgments

I am indebted to all mylab mates for their contributions to myknowledge and awareness in my research area, especiallyJerryPratt and Dr. Robert Ringrose who never got tired of answering all my doubts and helping me when I ran into problems. I also thank Jerryfor designing and building the planar biped ^Spring Flamingo~ which allowed me to set an application target for myresearch. I would also like to thank all the present and former lab members who contributed to the design of the simulation package, especiallythe Creature Library, without which myresearch would be verytedious. Thanks also to Peter

Dilworth and Jerryfor adding terrain features in the simulation package. I wish to thank myadvisor,

Prof. Gill A. Pratt, for letting me take on this research and giving me the freedom to undertake it. I also wish to thank Prof. Jean-Jacques Slotine for being the reader for this thesis in spite of his tight schedule. I would like to thank Jerry, Dave Robinson and Prof. Pratt for proof reading mythesis. Mywork at MIT would never have happened without the sponsorship of the National Universityof Singapore. I wish to thank mywife and daughter for being veryunderstanding and for providing me with moral support just at the right moment. I am also verygrateful to God, the Creator or Mother Nature for creating the physical world which is imbued with an uncountable number of intriguing phenomena and laws for us to explore.

Contents

1 INTRODUCTION ................................ ................................ ................................ ................................ 8

1.1 B

ACKGROUND ................................ ................................ ................................ ................................ .. 8

1.2 P

REVIOUS WORK ................................ ................................ ................................ .............................. 9

1.3 O

BJECTIVE AND S COPE ................................ ................................ ................................ ................... 10

1.4 O

UTLINE OF THE THESIS ................................ ................................ ................................ .................. 10

2 SEVEN-LINK PLANAR BIPED ................................ ................................ ................................ ....... 12

3 VIRTUAL MODEL CONTROL ................................ ................................ ................................ ....... 15

3.1 T

ASK CHARACTERISTICS AND SPECIFICATIONS FOR STEADY DYNAMIC WALKING OF A BIPED ................ 15

3.2 C

ONCEPT OF V IRTUAL M ODEL C ONTROL ................................ ................................ ........................ 16

3.3 A

PPLICATION TO STEADY DYNAMIC WALKING OF BIPED ................................ ................................ .... 17

3.3.1 Walking control using the state machine ................................ ................................ ................ 19

3.3.2 Swing leg strategy ................................ ................................ ................................ .................. 21

3.3.3 Key parameters ................................ ................................ ................................ ...................... 21

4 ROBUST ADAPTIVE CONTROL ................................ ................................ ................................ ... 26

4.1 B

ACKGROUND ................................ ................................ ................................ ................................ 26

4.2 T

HEORY ................................ ................................ ................................ ................................ ........ 26

4.3 A

PPLICATION OF R OBUST A DAPTIVE C ONTROL TO BIPED WALKING ................................ ................... 28

4.4 S

IMULATIONS RESULTS ................................ ................................ ................................ ................... 30

4.4.1 Effect of

l ................................ ................................ ................................ ............................ 30

4.4.2 Effect of k ................................ ................................ ................................ ............................... 31

4.4.3 Effect of D ................................ ................................ ................................ .............................. 32

4.4.4 Effect of g ................................ ................................ ................................ ............................ 32

4.4.5 Effect of

� m o ................................ ................................ ................................ .......................... 32

4.5 D

ISCUSSION ................................ ................................ ................................ ................................ ... 36

4.6 C

ONCLUSION ................................ ................................ ................................ ................................ . 36

5 SLOPED TERRAIN WALKING ................................ ................................ ................................ ...... 37

5.1 S

LOPED TERRAIN WALKING USING V IRTUAL M ODEL C ONTROL ................................ ......................... 38

5.1.1 Upslope and downslope walking ................................ ................................ ............................. 38

5.1.2 Transition cases ................................ ................................ ................................ .................... 41

5.2 E

XTENSION TO DYNAMIC STAIR - WALKING ................................ ................................ ....................... 46

6 SIMULATIONS RESULTS ................................ ................................ ................................ ............... 47

6.1 S

LOPED TERRAIN PROFILES USED IN THE SIMULATIONS ................................ ................................ ..... 47

6.2 W

ALKING OVER THE SLOPED TERRAIN PROFILE ONE ................................ ................................ ......... 48

6.3 W

ALKING OVER THE SLOPED TERRAIN PROFILE TWO ................................ ................................ ......... 53

6.4 W

ALKING ON STAIRS ................................ ................................ ................................ ...................... 56

6.5 D

ISCUSSION ................................ ................................ ................................ ................................ ... 58

7 CONCLUSIONS AND FURTHER WORK ................................ ................................ ...................... 60

7.1 C

ONCLUSIONS ................................ ................................ ................................ ................................ 60

7.2 F

URTHER W ORK ................................ ................................ ................................ ............................. 60

APPENDIX A: EQ UATIONS TO CONVERT VIRTUAL FORCES TO JOINTS´ TORQ UE

APPENDIX B: STABILITY ANALYSIS BASED ON "MASSLESS LEGS" MODEL

List of Figures

F IGURE 1. B

IPED ROBOT : ^S

PRING F LAMINGO ~ ................................ ................................ ....................... 12

F IGURE 2. S

EVEN - LINK PLANAR BIPED MODEL ................................ ................................ .......................... 13

F IGURE 3. V

IRTUAL M ODEL C ONTROL APPLYING TO TWO - LINK MANIPULATOR (P OSITION CONTROL ) .......... 17

F IGURE 4. V

IRTUAL COMPONENTS USED FOR BIPED WALKING ................................ ................................ .... 18

F IGURE 5. S

TATE DIAGRAM FOR WALKING CONTROL ................................ ................................ ................. 20

F IGURE 6. G

EOMETRIC CONSTRAINT FOR CALCULATING Z

LIMIT

................................ ................................ .... 23

F IGURE 7. M

ASSLESS LEG MODEL FOR THE BIPED ................................ ................................ ...................... 29

F IGURE 8. R

OBUST A DAPTIVE C ONTROL APPLIED TO Z - DIRECTION ................................ ............................ 30

F IGURE 9. R

OBUST A DAPTIVE C ONTROL : l =0.2, K =50, g =10, D=5,

�m o =9 ................................ ............ 33

F IGURE 10. R

OBUST A DAPTIVE C ONTROL : l = 2, K =50, g =10, D=5, �m o =9 ................................ ........... 33

F IGURE 11. R

OBUST A DAPTIVE C ONTROL : l = 5, K =50, g =10, D=5, �m o =9 ................................ ........... 34

F IGURE 12. R

OBUST A DAPTIVE C ONTROL : l = 10, K =50, g =10, D=5, �m o =9 ................................ ......... 34

F IGURE 13. R

OBUST A DAPTIVE C ONTROL : K = 100, l =2, g = 10 , D =5, �m o =9 ................................ ....... 34

F IGURE 14. R

OBUST A DAPTIVE C ONTROL : K = 500, l =2, g = 10 , D =5, �m o =9 ................................ ....... 34

F IGURE 15. R

OBUST A DAPTIVE C ONTROL : D = 0.01, l

= 2, K =50, g =10, �m o =9 ................................ ... 35

F IGURE 16. R

OBUST A DAPTIVE C ONTROL : D = 20, l

= 2, K =50, g =10, �m o =9 ................................ ...... 35

F IGURE 17. R

OBUST A DAPTIVE C ONTROL : g = 50, l

= 2, K =50, D =5 , �m o =9 ................................ ......... 35

F IGURE 18. R

OBUST A DAPTIVE C ONTROL : �m o = 13, l

= 2, K =50, g =10, D =5 ................................ ....... 35

F IGURE 19. F

OUR TYPICAL GEOMETRIES OF TERRAIN : ( A ) A GRADIENT ( B ) A DITCH ( C ) A VERTICAL STEP ( D )

AN ISOLATED WALL [S ONG AND W ALDRON , 1989] ................................ ................................ ............. 37

F IGURE 20. G

EOMETRIC CONSTRAINT TO CALCULATE H

LIMIT : L EVEL AND UPSLOPE ................................ ...... 40

F IGURE 21. G

EOMETRIC CONSTRAINT TO CALCULATE H

LIMIT

DURING DOWNSLOPE WALKING : ( A ) CASE 1; ( B )

CASE 2 ................................ ................................ ................................ ................................ ............. 41

F IGURE 22. N

ATURAL COMPLIANCE OF THE SWING FOOT ................................ ................................ ........... 42

F IGURE 23. ( A ) G LOBAL SLOPE WHOSE GRADIENT IS DIFFERENT FROM THAT OF THE ACTUAL SLOPE ; AND ( B )

GLOBAL SLOPE WHOSE GRADIENT IS THE SAME AS THAT OF THE ACTUAL SLOPE . ................................ ... 44

F IGURE 24. E

XTREME EXAMPLE TO DEMONSTRATE A POTENTIAL PROBLEM WHEN THE LOCAL SLOPE IS USED

TO CALCULATE THE DESIRED HIP HEIGHT . ................................ ................................ .......................... 44

F IGURE 25. S

EQUENCE FOR LEVEL - TO - DOWNSLOPE TRANSITION ................................ ................................ 45

F IGURE 26. P

OSSIBLE PROBLEM WITH SWING LEG ................................ ................................ ..................... 45

F IGURE 27. G

LOBAL SLOPE IN STAIR - WALKING ................................ ................................ ......................... 46

F IGURE 28. S

TICK DIAGRAM OF THE BIPED WALKING OVER THE SLOPED TERRAIN PROFILE ONE FROM LEFT TO

RIGHT ( SPACED APPROXIMATELY 0.08

S APART AND SHOWING ONLY THE LEFT LEG ) ............................. 50

F IGURE 29. P

ROFILES OF THE KEY VARIABLES WHEN THE BIPED WALKED OVER THE SLOPED TERRAIN PROFILE

ONE ................................ ................................ ................................ ................................ ................. 51

F IGURE 30. T

ORQUE PROFILES OF THE HIP AND THE KNEE JOINTS WHEN THE BIPED WALKED OVER THE SLOPED

TERRAIN PROFILE ONE ................................ ................................ ................................ ....................... 52

F IGURE 31. P

ROFILES OF THE KEY VARIABLES WHEN THE BIPED WALKED OVER SLOPED TERRAIN PROFILE TWO ..

................................ ................................ ................................ ................................ ....................... 54

F IGURE 32. V

ARIABLES ´ PROFILES OF THE BIPED WALKING OVER THE SLOPED TERRAIN PROFILE TWO USING

R OBUST A DAPTIVE C ONTROLLER AS THE VERTICAL VIRTUAL COMPONENT ( l = 2, K =100, g =10, D =5,

�m o =9) ................................ ................................ ................................ ................................ ............. 55

F IGURE 33. S

TICK DIAGRAM OF THE BIPED WALKING ON THE STAIRS ( SPACED APPROXIMATELY 0.2

S APART

AND SHOWING ONLY THE LEFT LEG ) ................................ ................................ ................................ .. 56

F IGURE 34. O

UTPUT VARIABLES PROFILES OF THE BIPED WALKING OVER THE STAIRS ................................ ... 57

List of Tables

T ABLE 1. I

NERTIA PARAMETERS OF THE SIMULATED BIPED ................................ ................................ ........ 14

T ABLE 2. L

ENGTH PARAMETERS OF THE SIMULATED BIPED ................................ ................................ ........ 14

T ABLE 3. D

ESCRIPTIONS OF THE STATES USED IN THE BIPED WALKING CONTROL ................................ ........ 20

T ABLE 4. G

AITS ´ PARAMETERS ................................ ................................ ................................ ................ 21

T ABLE 5. P

ARAMETERS OF VIRTUAL COMPONENTS ................................ ................................ .................... 21

T ABLE 6. D

ESIRED VALUES OF SOME OF THE GAITS ´ VARIABLES AND THE PARAMETERS OF THE VIRTUAL

COMPONENTS SET IN THE SIMULATION ................................ ................................ ............................... 48

C h a p t e r

1 Introduction

1 .1 Background

Biped locomotion is a hot area in legged locomotion research. One reason is that humans are themselves bipedal creatures and we hope to gain better insight into howhuman beings walk and run.

Another reason is that bipeds provide a great control challenge for engineers and scientists. Compared with robots that have more than two legs, bipeds usuallyhave a lesser number of actuators, and hence they are lighter in weight and lower in cost. Theyalso require a smaller foothold area for locomotion and thus are more versatile.

The task of controlling a biped to walk statically is easybut the resulting motion is slow. However, a control algorithm for it to walk dynamically is usuallycomplex and requires heavycomputation. Past researchers have tried to model biped locomotion using methods like Lagrangian or Newton-Euler mechanics. The resulting dynamic equations for the models were usuallyof high order and needed to be simplified bysome assumptions before a control technique could be applied. For example, [Furusho and

Masubuchi, 1986] derived the full equations of motion for a five-link planar biped and then linearized them around the vertical equilibrium and partitioned the linearized state equations into dominant and fast modes. The dynamics of the fast modes were ignored and proportional plus derivative feedbacks were applied at individual joints to track prescribed angular displacement profiles. The trajectorytracking was carried out in the joint space. [Kajita and Tani, 1991] studied a planar biped which was modelled as a massive bodywith two massless legs. The biped was controlled to walk in a mode called ^Linear Inverted

Pendulum~.

A control methodologycalled ^Virtual Model Control~ (VMC) [Pratt, 1995] was recentlydeveloped for legged robots. This method is based on intuition. The resulting controller does not need the dynamics information in order for a legged robot to perform steady 1 dynamic walking. Thus, it allows a computationallyless intense framework for the control since it does not require the computation of inverse dynamics for the legged robot. [Pratt, 1995] has successfullyused the VMC to control a planar biped to walk on flat ground.

1 Meaning the average horizontal velocityis constant.

Most research on biped locomotion has been restricted to level ground locomotion. Fewhave implemented bipeds that could walk on rough terrain. Without the capabilityof adapting to rough terrain, anylegged machine will defeat the purpose of its existence since the abilityto adapt to rough terrain is one of the most important reasons for legged locomotion. This provides us with a verygood motivation to extend the VMC to rough terrain locomotion of a biped.

1 .2 Previous work

[Zheng and Shen, 1990] have done research on a biped (SD-2) which walked on a slope in a statically stable way. The biped had force sensors at the feet to detect the transition of the supporting terrain from a flat floor to a slope and used a compliant motion scheme to adapt the landing foot to an unknown terrain.

Joint positions were then used to calculate the inclination of the landing foot as well as the slope gradient.

Theyfound that the slope walking of the biped involved simple modifications to a level walking gait.

Theysimplymodified the torso´s pitching angle so that the center of gravityof the biped was shifted to the most stable 2 position. Theyalso developed a transitional walking gait for SD-2 to walk from level ground to a slope, and vice versa. The same walking gait could be used for walking on level ground or on a slope.

The implementation of the strategywas simple. However, it was onlyapplied to static walking which had a slow locomotion speed.

[Yamaguchi, et al., 1996] introduced an anthropomorphic dynamic biped walking robot (WL-12RVII) which could adapt to a humans´ living floor. The biped had a special foot system (WAF-3) which was used to obtain a position relative to a landing surface and the gradient of the surface during its dynamic walking. The biped used an ^adaptive walking control system~ to adapt to path surfaces with unknown shapes byutilizing information concerning the landing surface obtained bythe foot system. The biped was able to perform dynamic walking and yet adapt to a humans´ living floor with an unknown shape.

The maximum walking speed was 1.28 s/step with a 0.3 m step length, and the adaptable deviation range was from -16 to +16 mm/step in the vertical direction, and from -3 o to +3 o for the tilt angle. These capabilities of the biped could be attributed mainly to the extensive design of the feet.

[Kajita and Tani, 1995] used a scheme called ^Linear Inverted Pendulum Mode~ to control a biped walking on rough terrain. Theydeveloped a simple control method for the biped byignoring the mass of the legs. Theyassumed that the biped knewthe profile of the ground in advance. Based on the predetermined foothold position for each step, a constraint line was calculated. The biped tried to follow the constraint line while keeping its body upright.

2 In the static sense.

1 .3 Objective and Scope

The objective of this thesis is to studythe feasibilityof applying the VMC to a planar 3 biped so that it can walk over slopes dynamicallywithout knowing the gradients and the transition positions in advance.

We wish to achieve the task byusing the signals from two discrete ground contact sensors located at the bottom of the biped´s feet. We also wish to achieve this task by simple modifications to the algorithm for level ground walking [Pratt, 1995]. The thesis will verifythe modified algorithm bysimulating a planar seven-link biped walking over sloped terrain.

The followings are the assumptions made in all the simulations:

1. It is assumed that the friction will be high enough to prevent anyslippage once the feet touch the ground.

2. It is assumed that the biped has perfect actuators which provide desired torque at each joint. In real systems, ^Series Elastics Actuators~ [Pratt and Williamson, 1995] are used to provide the desired torque at each joint.

3. The sloped terrain does not have step variations and the transition location between two different slope gradients is smooth. There is also no variation of terrain in the transverse direction.

1 .4 Outline of the thesis

Chapter 2 describes the configuration and parameters of the biped simulation model used in this thesis. The model is based on a physical planar seven-link biped called ^Spring Flamingo~.

Chapter 3 describes the basic idea of Virtual Model Control and its application to the biped. It then gives qualitative descriptions of the key parameters for walking control of the biped.

To maintain a nominal height of the biped when there is a change in the load applied onto it, Robust

Adaptive Controller [Slotine and Coetsee, 1986] is introduced into the control algorithm in Chapter 4 .

Several simulation results are included for the study of the effect of Robust Adaptive Control´s parameters.

Chapter 5 includes a strategydeveloped for the sloped terrain walking of the biped. This strategy allows the biped to walk blindlyover a series of slopes. It also explains howthe same strategycan be extended to stair climbing.

3 Constrained to move in sagittal plane only.

Chapter 6 includes all the simulation results of the sloped terrain walking of the biped. It also includes stair climbing simulation results. These results are used to validate the strategydeveloped in

Chapter 5. A general discussion is included at the end of this chapter.

Chapter 7 includes the conclusions and the future work that can be extended from this thesis.

C h a p t e r

2 Seven-linkPlanar Biped

In most control problems, the control methods adopted usuallydepend on the particular design of the plant. This is also true for biped locomotion. The control strategies studied in this thesis are designated for a physical six-d.o.f. seven-link planar biped called ^Spring Flamingo~ (see Figure 1 ) which was designed and built recentlybyJerryPratt in the Leg Laboratory 4 . It has two slim legs and a torso. Each leg consists of a hip joint, a knee joint and an ankle joint. All the joints are revolute pin joints with axes perpendicular to the sagittal plane.

Each joint has a rotarypotentiometer attached to measure the relative angles between two adjacent links. The relative angular velocityis obtained byan analog differentiator mounted on board the biped.

The pitch angle of the biped´s torso is measured bya rotarypotentiometer attached between the boom 5 and the torso. Each foot has two discrete sensors, one of which is positioned at the toe and the other at the heel. The sensors´ outputs are used to determine whether the biped´s foot is fullytouched down, heel down only, toe down only, or foot in the air.

Figure 1 . Biped robot: ^Spring Flamingo~

4 One of the research group belonging to the AIlab of MIT.

5 This is used to constrain the biped to walk in a circle.

z

x l c3 m 3 ,I 3

m 2 ,I 2

m 1 ,I 1 l c2 l c1

l 1 l 2

Figure 2 . Seven-link planar biped model

If we assume that during the single support phase, the ankle of the swing leg is fixed and there is no

actuation at the ankle of the stance leg, the dynamic equations for the biped during the single support

phase is similar to those derived in [Furusho and Masubuchi, 1986] for a five-link planar biped.

An equivalent computer model (as shown in Figure 2 ) was created and it has approximatelythe same

configuration and mass distribution as Spring Flamingo . The parameters of this model are tabulated in

Table 1 and Table 2 .

The simulation environment mainlyconsists of a dynamics simulator package (SD-FAST 6 ) and a

proprietarysoftware library. The proprietarysoftware librarywas written bypast and present affiliates of

Leg Lab. It includes functions for model creation (Creature Library), ground contacts specifications,

terrain specifications, etc.. After setting up the computer model for the biped, the user is required to

design a control algorithm in C code. The control function is called every^ control dt_ ~ seconds to

supply the desired torque or forces to the model´s actuators.

6 Product of Symbolic Dynamics.

Table 1 . Inertia parameters of the simulated biped

Part Mass (kg) Moment of inertia about the center

of mass, I yy (kg m 2 )

Torso 10.0 3 4 1 1 0 2 . ´ -

Upper leg link 0.460 1 3 0 1 0 4 .´ -

Lower leg link 0.306 5 7 0 1 0 5 .´ -

Foot 0.251 3 7 0 1 0 4 .´ -

Total mass 12.03

Table 2 . Length parameters of the simulated biped

Description Value

Torso

Height of center of mass referred from hip, l c3 0.2 m

Upper leg link

Length of upper leg link, l 2 Distance of center of mass of the upper leg from the knee joint, l c2

0.42 m

0.117 m

Lower leg link

Length of lower leg link, l 1 Distance of center of mass of the lower leg from the ankle joint, l c1

0.42 m

0.238 m

Foot (Symmetrical)

Foot length

Distance from ankle joints to foot based

0.15 m

0.04 m

C h a p t e r

3 Virtual Model Control

In biped locomotion, it is generallydifficult to transform from high level task specifications, such as

^walk forward~ to lowlevel motion control such as the required joint torques or trajectories. Furthermore,

the dynamic equations of a biped are usuallyof high order. Even if we can derive the dynamic equations

for the biped, we still face the problem of underactuation at the ankle during single support.

In the implementation of biped walking, one common approach is to compute and command the joint

space trajectories at each phase of the walking gait and this is mostlybased on a desired trajectory(e.g. of

the body) in the cartesian space or some pattern generators, etc.. The desired joints´ trajectories can be

achieved bynonlinear control techniques like computed torque control [Mitobe et al., 1995] , robust

control [Tzafestas et al., 1996] , adaptive control [Yang, 1994], etc.. However, this wayof controlling a

biped is computationallyintensive as we need to compute the inverse dynamics. To avoid such

complexity, some researchers linearize the nonlinear dynamic equations of the biped and apply modern

control techniques .

The Leg Laboratory has developed a newcontrol approach called Virtual Model Control (VMC) for

the implementation of legged locomotion. The framework of this approach was well defined in [Pratt,

1995] and a comparison with other techniques like Impedance Control , Stiffness Control etc. was also

included. This chapter gives a brief introduction to this approach and elaborates the details used bythe

biped to perform steadydynamic walking on level terrain. It will also provide a qualitative description of

the control parameters. This approach will be extended to sloped terrain walking in Chapter 5.

3 .1 Task characteristics and specifications for steady dynamic walking of a biped

Before we decide on the control approach to a system, it is important to first examine the desired task

for the system. This thesis assumes that the task goal for the biped described in Chapter 2 is to realize a

steadydynamic walking gait in the sagittal plane, while maintaining an upright posture for the torso. It

also assumes that the walking gait consists of two main phases: single support and double support. Note

that when the biped is in the single support phase, it is inherentlyunstable (just like an inverted

pendulum) due to the gravityforce. Thus, it is not possible to track anyarbitrarytrajectoryas in a

manipulator arm even if it is within the non-singular workspace. The stabilityof the biped is maintained

by alternating between the left and right support phases in the right cycle.

One characteristic of natural biped walking is that the exact trajectoryof the torso is not important.

For example, in human walking, we usuallydo not specifya walking task bynumbers. We simplytryto

maintain a generallyupright position and interact with gravityand ground friction to perform stable

walking. The specification for the horizontal walking velocityis always fuzzy. For example, we think in

terms of ^fast~, ^medium~, ^slow~ motion etc.. It has been shown that a planar biped can walk passively

down a gentle slope without any actuators [McGeer, 1990].

In this thesis, we specifythe desired height and velocityof the torso, while keeping it in an upright

position. However, the height and horizontal velocityare allowed to varywithin a tolerable range. So,

the next question is whether we need a verycomplex and precise dynamic model for the biped to achieve

such specifications. The next section describes a simple method called Virtual Model Control which has

been successfully implemented on a five-link planar biped permitting it to walk steadily on level ground.

3 .2 Concept of Virtual Model Control

In Virtual Model Control (VMC) [Pratt, 1995], we use virtual components (e.g. springs, dampers etc.)

to generate the required actuators´ forces. Byattaching virtual components (which usuallyhave

corresponding physical parts, for example, a spring and a damper) at some locations of the biped, the

biped will behave dynamicallyas if the actual physical components are attached to it provided that the

actuators are perfect 7 .

Virtual Model Control approach results in a control algorithm which examines the virtual components

to obtain virtual forces from their constitutive equations. Then these forces can be transformed to the

actuator space bya transformation matrix. Bychanging the set points of the virtual components, we

create an inequilibrium to the system; it will then adjust itself so that a newequilibrium position is

reached.

The main mathematical data used in this approach is the Jacobian transformation matrix which relates

the force vector in one space to another space. For example, in robotics application, we usuallytransform

a force vector

& F in the cartesian space to an equivalent torque vector

�

- q 2 q 1

Figure 3 . Virtual Model Control applying to two-link manipulator (Position control)

3 .3 Application to steady dynamic walking of biped

In the implementation of biped walking using the VMC, the placements of virtual components require intuition; there maybe more than one set of virtual components to achieve the global task defined in

8 Those which have the same constitutive properties as the virtual components.

Section 3.1 . Since we are interested in the motion described in cartesian space, it is natural for us to attach virtual components along each of the orthogonal coordinates in this space. One possible set of virtual components (same as those used by[Pratt, 1995]) is shown in Figure 4 . A virtual spring-damper is attached to the hip along the vertical direction to generate a virtual vertical force F z at the hip. It is used to control the vertical height of the biped. A virtual damper is attached to the hip along the horizontal direction to generate a virtual horizontal force F x at the hip. This is used to control the horizontal velocityof the biped. A rotational spring-damper is attached at the hip to generate a virtual rotational force M a about the hip. This is used to maintain the upright posture of the biped´s torso. The legs of the biped are bent towards the back during walking. That is, the biped walking bears more resemblance to birds than to humans.

Though the biped has actuated ankles, we set the ankle of stance leg to be limp bycommanding a zero torque. This results in a motion similar to that of the previous 5-link biped [Pratt, 1995] which had no feet. The feet of the 7-link biped simplyprovide better traction during the single support phase. The usage of the ankle of the stance leg to modifythe walking gait is beyond the scope of the thesis, but it has been implemented in the Leg Laboratory by Jerry Pratt.

l c3

m 3 ,I 3 m 2 ,I 2 m 1 ,I 1

l c2 l c1 l 1

l 2

v x xd d or

�

Z

X O

x b

z b o b

Frictionless

Figure 4 . Virtual components used for biped walking

For our biped walking control, the inputs are the desired horizontal velocity

�x d (or v xd ), the desired vertical height of the hip z d and the desired pitch angle of the body

a d . All these inputs define the

desired motion of the bodyframe O b X b Z b with respect to the inertia frame OXZ. Assuming the virtual

components are linear, we can obtain the following control law in the cartesian frame:

F b x x

x x d

: ( � � )

= - (3.2)

F k z z b z z

z z d z d

: ( ) ( � � )

= - + - (3.3)

M k b d d a a a a a a a : ( ) ( � � )

= - + - (3.4)

where b i and k i are the damping coefficient and the spring stiffness, respectivelyfor the virtual

components in i (= x , z or a ) coordinate.

However, this set of virtual components can onlybe applied to the double support phase and not to the

single support phase. During the single support phase, since we have set the ankle of the stance leg to be

limp, the biped loses one actuated degree of freedom. Thus, one of the virtual components cannot be

realised. We chose to maintain the vertical and rotational spring-dampers and let the interaction between

gravity and these virtual components dictate the horizontal velocity during this phase.

The virtual forces for both the single and the double support phases are transformed into the joint

space using the equations derived in [Pratt, 1995]. A list of the equations can be found in Appendix A.

Realtime control of the biped locomotion can be implemented based on a state machine and the equations.

In this way, the VMC enables the biped to walk without computing the inverse dynamics and kinematics

and hence simplifies the computation significantly.

3 .3 .1 Walking control using the state machine

The pattern of events, states, and state transitions of the biped walking can be represented bya state

diagram ( Figure 5 ). The states listed in Table 3 are used to identifydistinct phases of control in a walking

cycle. A software finite state machine is used to synchronise the state transitions bymonitoring for some

specified conditions in the sensorydata. Note that such implementation provides organised handling of

the sensorydata, but it does not provide a foolproof solution unless we include all the possible discrete

states in the algorithm.

Table 3 . Descriptions of the states used in the biped walking control

State Description

1. Double Support 1 Both feet are on the ground. Right foot is in

front.

2. Right Support The right foot is the stance leg and the left

foot is the swing leg. Neither switch of the

left foot is activated. The distance between

the swing leg and the stance leg is less than

the step length.

3. Single-to-Double Transition 1 This is the intermediate phase where Right

Support state transits to Double Support 2.

4. Double Support 2 Both feet are on the ground. Left foot is in

front.

5. Left Support The left foot is the stance leg and the right

foot is the swing leg. Neither switch of the

right foot is activated. The distance between

the swing leg and the stance leg is less than

the step length.

6. Single-to-Double Transition 2 This is the intermediate phase where Left

Support state transits to Double Support 1.

DOU BLE_SUPPORT_1

(1)

RIGHT_SUPPORT

(2)

SINGLE_TO_DOUBLE

_TRANSITION_1

(3)

DOU BLE_SUPPORT2

(4)

LEFT_SUPPORT

(5)

When transition point is reached

1. One of the limit switches of the swing foot

is activated; or

2. The step length is reached

Left foot has completely touched down

SINGLE_TO_DOUBLE

_TRANSITION_2 (6)

When transition point is reached

Right foot has completely touched down

1. One of the limit switches of the swing foot

is activated; or

2. The step length is reached

Figure 5 . State diagram for walking control

3 .3 .2 Swing leg strategy

In the steadywalking control considered in this thesis, the objective of a swing leg strategyis to

achieve approximatelythe desired step length. When the swing leg touches down, we also want the

vertical projection of the hip to be approximatelyat the center between the feet. The two keyvariables of

the swing leg task are the desired step length s l and the desired lift height h l . These two variables will

be discussed in the next subsection. The detailed control strategyfor the swing leg is beyond the scope of

this thesis.

3 .3 .3 Key parameters

This section highlights the keyparameters that mayaffect the walking pattern and performance of the

planar biped. Theyare mainlydivided into gaits´ ( Table 4 ) and virtual components´ ( Table 5 )

parameters. This subsection provides a qualitative discussion of these parameters.

Table 4 . Gaits´ parameters

Parameter Notation

Desired pitch angle of the torso a d Desired hip height z d Desired horizontal velocityof the hip v xd Desired step length s l Distance from the front ankle at which double

support phase transits to single support phase l t

Swing leg :

a) Desired lift height h l b) Swing time t s

Table 5 . Parameters of virtual components

Parameter Notation

1. Spring stiffness (in z direction) k z

2. Damping coefficient (in z direction) b z

3. Damping coefficient (in x direction) b x

4. Spring stiffness (in a direction) k a

5. Damping coefficient (in a direction) b a i) Desired pitch angle of the torso, a d

This variable is used directlybythe torsional virtual spring-damper. The simulated biped has a torso

whose center of gravityis above the hip joints. Bychanging the maintained pitch angle of the torso, the

projection of the overall biped´s center of gravitycan be shifted. When ascending a slope, the natural

reaction for a human is to lean forward. When descending a slope, he naturallyleans back as depicted by

the photographs in [Muybridge, 1989]. However, to simplifymatters, the desired pitch angle of the torso

is set at zero degree in this thesis regardless of the slope gradient.

ii) Desired horizontal velocity at the hip, v xd

In biped walking, several approaches can be adopted to maintain the desired horizontal velocity. For

example, we can control the horizontal velocityof a biped byfoot placement [Raibert, 1986] as in the case

of a hopping machine. In walking, we have a period where both feet are on the ground (double support)

and this also can be utilised for horizontal velocity control.

In the previous analysis, we utilised a horizontal virtual damper to correct the horizontal velocity.

Since the ankle torque is zero, the biped can onlyhave this control (without sacrificing the vertical height

and bodypitch control) when it is in the double support phase. To prevent the divergence of the

horizontal velocity, we want the double support dutycycle to be as large as possible. However, this

approach to maintain the horizontal velocitymaynot be effective if the walking speed is high. This is

because the actual duration of double support is veryshort during high speed walking. Also, although the

equations developed in [Pratt, 1995] assumed that full horizontal force can be achieved during double

support, this is not true in real applications since the foot of the biped is not hinged to the ground. Thus,

we need to set a limit to the horizontal virtual force due to the virtual damper.

We can also modulate horizontal velocitybyvarying the transition position from double to single

support. In single support, we want to have a swing leg control strategythat minimises the disturbance to

the horizontal velocity.

iii) Desired hip height, z d

If the biped is in double support phase, the desired hip height is defined with respect to the ankle joint

of the back supporting leg. Otherwise, it is defined with respect to the ankle joint of the stance leg. This

variable is used bythe vertical virtual spring-damper to compute the desired vertical force at the hip. At

the singular configuration in which the stance leg or one of the legs during double support is fully straightened, although the transformation equations do not ^blowup~, the dynamics of the system is

unpredictable. Thus, it is veryimportant to select a proper hip height so that the leg of the biped will not

reach the singular configuration. The upper limit is set bythe geometryof the legs and the desired step

length. This variable should not be too small since it will increase the required knee torque and hence the

the energyto maintain the biped´s height. This is due to the increase in the moment arm of the body

weight with respect to the knee joints. Thus, we would like to have this variable close to the upper limit

but not reaching it.

In the algorithm, the upper limit of the hip height z limit was computed as in Equation (3.5):

z l l l

limit

= + - ( ) 1 2 2 2 (3.5)

where l s l l t = + , s l is the desired step length and l t is the distance from the front ankle at which the

double support phase transits to the single support phase.

We usuallyset the desired height at a fraction of this limit (using a factor k hei ght

=0.8~0.9) to cater to

anydiscrepancyin the actual hip height and the actual step length. This will also allowthe biped to better

accommode unknown terrain variations. Note that the foot´s dimension is ignored in the computation

since we compute everything with respect to the cartesian frame attached to the ankle.

l 1 +l 2

z limit

l

Transition plane

Figure 6 . Geometric constraint for calculating z limit

iv) Desired step length, s l

This variable is used to plan the trajectoryof the swing leg. It is coupled to the hip height as discussed

before. We usuallychoose a desired step length depending on the lengths of the legs’ links. In our

present approach the double support phase is used mainlyto correct the horizontal velocity. The step length affects the relative period of the double support phase compared to the single support phase. Thus,

this parameter indirectly affects the ^controllability~ of the horizontal speed of the locomotion.

v) Distance from the front ankle at which double support phase transits to single support phase, l t

This is the projected horizontal distance of the hip from the ankle of the front leg where the biped

changes from the double support phase to the single support phase. It should be forward enough so that

the biped will not lose too much energyduring the single support phase, otherwise it maylose all its

forward momentum. It should not be forward to the extent that the forward velocityincreases excessively

after a single transition. The walking cycle maybecome unstable if the transition position is not properly

selected.

vi) Lift height, h l (For swing leg control)

This variable corresponds to the maximum lifting height of the swing leg during the swing motion and

it is used in the trajectoryplanning of the swing leg. It mayindirectlyaffect the degree of disturbance on

the torso created bythe swing leg. Its value is critical if the premature landing of the swing leg (e.g. in

stair climbing) is undesirable.

vii) Swing time, t s (For swing leg control)

This variable corresponds to the time available for the biped to swing its leg during the single support

phase. This is calculated approximatelyfrom the velocityat the hip before the double to single support

transition. As discussed in subsection 3.3.2 , we want the hip of the torso to be roughlyat the center,

between the front and back supporting legs at touch down of the swing leg.

viii) Parameters of the virtual components

These parameters are tuned bytrial and error. Some intuition based on the linear system helps too.

For example, for the vertical virtual spring-damper, we would like to have sufficientlyhigh spring

stiffness for a sufficientlyquick response. The damping coefficient is then adjusted so as to achieve

overdamped response. The tuning process can be iterated if required. In actual implementation, the

response of the virtual component is limited bythe bandwidth of the actuators. Such an approach for

tuning also applies to the rotational virtual spring-damper. Note that although the virtual spring-dampers

are linear components, the resulting dynamic system is nonlinear. Hence, it is not desirable to have

oscillatory motion in the resulting system as nonlinear oscillatory motion can be non-intuitive.

The tuning of the horizontal virtual damper is less stringent. It can be tuned after the other virtual

components are done. As mentioned before, we have to set a limit to the virtual horizontal force

generated by this virtual damper because the feet are not hinged onto the ground.

C h a p t e r

4 Robust Adaptive Control

4 .1 Background

In the walking control of the planar biped, the previous chapter has demonstrated that a virtual spring-

damper in the vertical direction can be used to control height. In the actual implementation, a constant

offset term is added to compensate for the effective weight of the biped as perceived at the hip so that the

biped can maintain close to the desired hip height without having a stiff virtual spring. However, it is not

able to adapt to a varying torso mass which mayoccur if it carries an external load. For example, the

biped will walk with a lower height if the torso´s weight is increased. A possible solution would be to

applyadaptive control in the joint space [Yang, 1994]. However, the inverse dynamics of a biped even in

the planar case is verycomplex. This is complicated bythe fact that in the single support phase, we lose

an actuated degree of freedom at the ankle especiallyif the ankle is limp. Inspired bythe VMC approach,

this chapter will perform a feasibilitystudyof the replacement of the existing vertical virtual component

by Robust Adaptive Controller developed by[Slotine and Coetsee, 1986]. The purpose is to enable the

biped to adapt to varying mass and walk with a height close to the desired value. The following sections

will describe the theoryof Robust Adaptive Control and howit can be applied to our biped to maintain its

hip height.

4 .2 Theory

This section includes the basic theoryof Robust Adaptive Control. Since we are interested in a

dynamics problem which is governed bythe Newton´s Second Law, let´s consider the following second

order nonlinear equation:

a x a f x x a g x d x x t u

1 2 3

� � ( � , ) ( ) ( , � , )

+ + + = (4.1)

where a 1 , a 2 and a 3 are unknown constants, f x x(

� , ) and g x( ) are nonlinear functions, d x x t( , � , ) is

the disturbance of known bound D (i.e. d D£ ) and u is the input.

Definitions:

s t x x x x r ( ) ~� ~ � � = + = - l , (4.2) where ~ z z z d = - , � � ~ x x x r d = - l and l is a strictly positive constant.

s t s t sat s t

D ( ) ( ) (

( )

) = - f f (4.3)

The goal of the control is to make s D º 0 such that s is bounded by f . It can be shown that [Slotine

and Li, 1991]

" ³ £ Þ " ³ £ t s t t x t i i 0 0 2

, ( ) , ~ ( ) ( ) ( ) f l f

l , i =0,1. (4.4)

To ensure that s D ( ) ¥ ® 0 , let´s define

Y x f x x g x r = [ � � ( � , ) ( ) ] ,

[ ]

& a a a a T = 1 2 3 ,

& & & ~

� a a a

= - .

where & � a is the estimate of & a . We can choose the following Lyapunov candidate function

V a s a a T = + -

1 2 1

2

1

2 D G & & ~ ~ . (4.5)

where G is a symmetric positive definite constant matrix. The time derivative of V is then given by

� � � � ~

( � � � � ) � � ~

( � � ) � � ~

V a s s a a

s a x a x a a

s u a f a g d a x a a

T

r T

r T

= +

= - +

= - - - - +

-

-

-

1 1

1 1 1

2 3 1 1

D

D

D

G

G

G

& &

& &

& &

Let´s define the control law as

u Y a ks = - & � (4.6)

where k is a strictly positive constant. Then

� ~ � � ~ V s Y a s d ks s a a T = - - + -

D D D G & & & 1 .

By setting s Y a T D G + = - & � � 1 0 , we obtain the adaptation law

& � � a Y s T = - G D . (4.7)

Thus, � V becomes

� ( ( ))

V s d ks s sat s

s d ks k s

= - - +

= - - -

D D D

D D D f f

f 2

By setting k D f = , the resulting expression of �V is

� V ks £ - D 2 (4.8)

By Barbalat´s Lemma [Slotine and Li, 1991], we can show that s D ® 0 as t ® ¥ .

4 .3 Application of Robust Adaptive Control to biped walking

Based on the massless leg model as shown in Figure 7 , we applyRobust Adaptive Control to the z-

direction dynamic equation of the biped as shown below:

m z mg d p p t F z � � ( , � , ) + + = & & ( 4.9)

where m is the effective mass of the biped observed at the hip, & p x z T = [ , , ]a and d p p t ( , � , ) & & ( d D £ )

is the disturbance term which includes the variation 9 of the effective inertia and the effect of the swing leg

dynamics. Note that the resulting system in the z -direction can be viewed to be a new^virtual

component~ for the VMC ( Figure 8 ) which generates F z , while the other two variables ( v xd and a d ) are

still controlled using the virtual components described in Section 3.3 .

Definitions:

� � ~ z z z r d = - l , where ~ z z z d = - (4.10)

s z z z z r = + = -

~� ~ � � l (4.11)

s s sat s

D = - f f ( ) (4.12)

Ya z g m r = + ( � � ) (4.13)

where a m = and Y z g r = + (

� � )

9 Due to the variation in the effective weight of the legs as perceived at the hip.

The following control law (Equation (4.14)) and adaptation law (Equation (4.15)) are used:

F Y a ks z = -� (4.14)

� � a Y s T = - g D (4.15)

where g is a strictly positive scalar.

Note that, on level ground walking, � �z d = 0 and �z d = 0 . The following section studythe effects of

each variable ( l , k, g , D, �m o 10 ) used by this Robust Adaptive Controller.

l m,I

z

x z

b

x

b

- a

F

x

F

z

M

a

o o

b

Figure 7 . Massless leg model for the biped

10 This variable is the initial estimate for m .

l c3 m 3 ,I 3

m 2 ,I 2

m 1 ,I 1 l c2 l c1

l 1 l 2 v

xd

Robust

Adaptive

Control

z

x

+ a

Frictionless

Figure 8 . Robust Adaptive Control applied to z -direction

4 .4 Simulations results

In this section, the effects of the parameters ( l , k, g , D, �m o ) described in the previous section are

studied based on level ground walking simulation of the biped. In all the simulations, the desired height

of the hip was fixed at z d =0.7 m, the desired horizontal velocitywas fixed at v xd =0.4 m/s and desired pitch

angle was fixed at a d = 0 . The initial conditions of the simulation were assigned to be the same as the

desired value. The desired step length of the biped was fixed at 0.28 m.

4 .4 .1 Effect of l

We first varied l while setting the other parameters as follows: k =50, g =10, D =5, �m o =9. The

simulation results for l =0.2, 2, 5 and 10 are shown in Figure 9 , Figure 10 , Figure 11 and Figure 12 ,

respectively.

Theoretically, when s D ® 0 , ~ z will converge toward the bound ( f l ) (Equation (4.4)). Since

f = D k and both D and k were fixed in these simulations, large l would result in small ~ z . This is demonstrated to be true bycomparing the top graph of Figure 9 , Figure 10 , Figure 11 and Figure 12 .

Note that l also behaves like the ratio of the proportional gain over the derivative gain in a PD

controller. However, in a real system, l is limited bythe structural resonant modes, neglected time

delays and sampling rate [Slotine and Li, 1991]. Furthermore, for biped locomotion, the foot is not fixed

to the ground like that of a manipulator. So, we do not want l to be too high.

From the top graph of Figure 9 , we observed that when l was too low, the bound (= f l ) for

~ z became too big (Equation (4.4)) and the hip height fluctuated significantly. Due to the large fluctuation

in the hip height, the biped´s leg(s) reached singular configuration and resulted in instability.

It was observed that for all l ’ s used here, ~ z did not seem to converge to within the bound (given

by f l ). This might be due to the fact that the disturbance bound D we set was too small compared to the

real disturbances (e.g. due to the swing leg dynamics). That is, the results of the theoretical analysis we

have done do not hold if selected D is smaller than the actual D . Interestingly, it was also observed that

for l =2, ~ z remained positive after the transient response had subsided.

Since we have mentioned that in our biped walking control, exact trajectorytracking is not important,

the result of l =2 is acceptable and we set l =2 for the subsequent simulations. Besides, if l is too high,

it may cause the biped to be unstable if it walks on rough terrain.

4 .4 .2 Effect of k

Equation (4.14) shows that the value of k influences the effect of s on F z . k also directlyaffects f

(= D/k ), which in turn affects the bound for ~ z as discussed before. This subsection compares the

simulation results of Figure 10 , Figure 13 and Figure 14 to studythe effect of k . The top graph of these

figures verifies that as value of k increases, the bound for ~ z becomes smaller. Large k also improved the

transient response of ~ z because it acts like a gain to the controller. However, when k was increased, the

variation in the control input F z was veryhigh and abrupt (see the graph of F z vs x in Figure 10 , Figure 13

and Figure 14 ). Such variation in F z maynot be achievable in a real system if the required bandwidth is

much larger than the actuator´s bandwidth. Also, high k will retard the adaptation rate for �m (comparing

the graph of �m vs x in Figure 10 , Figure 13 and Figure 14 ) since the PD portion of the control law

(Equation (4.14)) dominates in the contribution to the control input F z .

4 .4 .3 Effect of D

The parameter D has direct influence on f (= D/k ). From the mathematical point of view, we want D

to be small. However, D is determined bythe actual disturbances. To studythe effect of D , this subsection

looks at the simulation results shown in Figure 10 , Figure 15 and Figure 16 .

Comparing the top graph of Figure 10 and Figure 16 , the results demonstrated that when D was large,

it indeed allowed a greater variation in ~ z . Also, for the s D plot, we observed that the larger was D , the

^quieter~ was s D after the initial transient response.

For verysmall D as in Figure 15 , we observed that �m was oscillatory. This was due to the adaptive

controller trying to adapt to the disturbances. In contrast, the result in Figure 16 shows that �m converged

smoothly to a constant value after some time.

4 .4 .4 Effect of g

g appears in Equation (4.15) and hence it is one of the parameters which affects the adaptation rate

for �m . It behaves like the gain of an integral controller. This subsection compares the simulation results

between Figure 10 and Figure 17 .

For higher g ( Figure 17 ), it was observed that ~ z was smaller at the transient portion. This was

because �m was being updated at a faster rate. However, after the transient portion of the response was

over, ~ z seemed to having the same behaviour and bound as shown in both figures. It was also observed

that for high g , �m became rather oscillatory(comparing the graph of �m vs x in Figure 10 and Figure

17 ).

4 .4 .5 Effect of

�m o (the initial value for �m ) so that it differed from the actual effective mass.

When �m o is smaller than actual effective mass (see Figure 10 where �m o =9kg), it corresponds to the instance when the biped just loads itself with an external load. When �m o is greater than actual effective mass (see Figure 18 where �m o =13kg), it corresponds to the instance when the biped just unloads an external load. The simulation results showed that the biped indeed had the capabilityof adapting to the changes in effective mass for both unloading and loading of an external load which was about 18% of the effective mass.

Note that the actual effective mass deviates from bodymass (=10kg) because the former includes the effective mass of the leg(s) too. In the biped walking simulation, although we knowthe bodymass, we do not have readyinformation about the effective mass of the leg. We need to obtain the inertial mass matrix referred to the hip and this is cumbersome. The properties of Robust Adaptive Control allows us to absorb part of the effective mass of the legs into �m and treat the rest of which as a disturbance.

Figure 9 . Robust Adaptive Control: l =0.2, k=50,

                                           g =10, D=5, �m

                                                                                      o
                                                                                           =9

Figure 10 . Robust Adaptive Control: l  = 2,
k=50, g =10, D=5, �m
o
=9

Figure 11 . Robust Adaptive Control: l  = 5, k=50,

                                            g =10, D=5, �m

                                                                                        o
                                                                                            =9

Figure 12 . Robust Adaptive Control: l  = 10,
k=50, g =10, D=5, �m
o
=9

       Figure 13 . Robust Adaptive Control:  k  = 100,

                                  l =2, g = 10 , D =5, �m

                                                                                                  o
                                                                                                      =9

Figure 14 . Robust Adaptive Control:  k  = 500,
l =2, g = 10 , D =5, �m
o
=9

Figure 15 . Robust Adaptive Control:  D = 0.01, l

                                    = 2, k=50, g =10, �m

                                                                                               o
                                                                                                   =9

Figure 16 . Robust Adaptive Control:  D = 20, l

= 2, k=50, g =10, �m
o
=9

 Figure 17 . Robust Adaptive Control: g  = 50, l  =

                                         2, k =50, D =5 , �m

                                                                                          o
                                                                                              =9

Figure 18 . Robust Adaptive Control:  �m
o
 = 13, l

= 2, k =50, g =10, D =5

4 .5 Discussion

          One may ask whether we can simply use PID controller instead of the more complex Robust Adaptive

Controller.  We would say that a PID controller will probably work fine too.  Nonetheless, we think that

Robust Adaptive Controller is better because it provides the information of the effective mass.

Furthermore, the computation of Robust Adaptive Controller is not very intensive and hence it is
worthwhile to implement Robust Adaptive Controller for our purpose.  In fact, when the estimation of m
has stopped and all other transient behaviors have settled down, Robust Adaptive Controller behaves like
a virtual spring-damper with a constant offset term (Equation (4.14)).

          If the legs are heavy, we may split the adaptation parameters into two parts, one for the single support
phase and the other for the double support phase because the effective mass for the two phases may
deviate substantially from one another.

4 .6 Conclusion

          This chapter has demonstrated successful application of Robust Adaptive Control to biped walking on
level ground in the simulation.  The effects of the parameters were also studied.  It is concluded that

Robust Adaptive Controller is applicable for steady biped walking and it enables the biped to adapt to
about 18% step  change in body mass.  The computation requirements for such a controller are very low
and do not defeat the original purpose of using the VMC.  Thus, Robust Adaptive Controller can be a
virtual component candidate for the VMC.  Chapter 6 will demonstrate the robustness of this approach by
simulating the biped walking over a series of unknown slopes.

C h a p t e r

5 Sloped terrain w alking

          In a totally unstructured environment, the geometry of the terrain is usually very complex.  In the
study of  rough terrain locomotion by a hexapod, [Song and Waldron, 1989] classified the rough terrain
into four types of geometric representations:  gradient, ditch, vertical step and isolated wall ( Figure 19 ).

[Raibert, 1990] said that a terrain can become rough under the following instances: 1) the ground is not
level; 2) there is limited traction (slippery); 3) there are areas of poor or nonexistent support (eg., holes).

                                                                         (a) a gradient (b) a ditch

                                                                    (c) a vertical step (d) an isolated wall

                            Figure 19 .  Four typical geometries of terrain: (a) a gradient (b) a ditch (c) a vertical step (d) an

                                                                                                          isolated wall [Song and Waldron, 1989]

          The types of terrain that a biped can overcome depend not only on the relative dimension between the
terrain and the biped, but also its mechanism, structure and walking gait.  So, when designing a biped, it
is very important to take into account the type of terrain it has to overcome.  However, this thesis assumes
that the biped is already designed and the task is to develop an algorithm for the biped to overcome certain
types of rough terrains.  This thesis will look only at gradient or sloped terrain.  The main objective is to
develop a simple  strategy for sloped terrain walking based on Virtual Model  Control (VMC) approach.

Based only on geometric considerations, we modified the algorithm for walking on level ground so that
the biped can walk on slopes.  Last, this thesis also extends the sloped terrain walking strategy to stair
climbing.  All the simulation results are presented in the next chapter.

5 .1 Sloped terrain walking using Virtual Model Control

          Within a building, be it a commercial, industrial or residential one, the terrain is usually well
structured and it can be classified mainly into level ground, slopes and stairs.  We will first consider the
slopes and extend the application of the VMC  to sloped terrain walking.  The biped  is assumed to be
walking on level ground before encountering a slope of unknown transition location and gradient .  The
biped is just like a blind creature and it should be able to adjust its gait based on its interaction with the
slope [Zheng and Shen, 1990] .

          This thesis assumes that the terrain has no vertical variation along the walking direction and no
variation perpendicular to the sagittal plane.  The minimum and maximum slope gradient s are -20 o  and

+20 o ,  respectively.  This thesis also assumes that there is no slippage of the feet at all time when they are
in contact with the ground.

          As mentioned in Chapter 2 , the biped in our study has only discrete sensors at the toe and heel to sense
the foot´s contact with the ground.  Together with the joints´ position readings, the information provided
by these discrete sensors is used to compute the slope gradients at the start of each double support state.

The biped will adjust its gait accordingly to continue its stable locomotion on the slope.  Since our biped
walks dynamically on level ground, we also want it to walk dynamically up or down the slope.  The
objective is to let the biped  adapt to the slope of unknown gradient without complex sensors and
algorithm.

          When the biped  is on a slope and it is in the double support phase, the front and rear supporting legs
are resting on different elevations.  We call the virtual slope that is formed by joining the ankle of the
front and rear legs the global  slope.  The actual slope that each foot is resting on  is called the local  slope.

For example, when the back supporting leg is stepping on level ground and the front supporting leg is
stepping on an upslope, the local slopes at both legs and the global slope will all have different gradients.

In the algorithm, the local and global slope gradients are computed during the double support state.

5 .1 .1 Upslope and downslope walking

          This subsection studies the posture of the biped while walking on an upslope and a downslope which
have constant gradients.  We then decide which parameters or variables should be adjusted so that steady
walking can be achieved.

          For the biped, the following are some of the possible strategies which can be adopted for slope
walking:

1.  To adjust the projection of the center of gravity of the biped along the ground.  For example, the biped

            may bend its torso forwards during upslope walking to shift the projection of the center of gravity

            forwards;

2.  To vary the hip height;

3.  To change the distance from the front ankle at which the double support phase transits to the single

            support phase;

4.  To vary the horizontal velocity;

5.  To vary the step length.

          These strategies may be used to improve the walking in one way or another, for example, in terms of
stability and energy usage.  Some of them may have opposing effects on the slope walking control and this
requires optimization methods to obtain an optimal solution.  However, we have not yet established a
performance index for steady dynamic walking on rough terrain.  Therefore we adopt trial-and-error
approach to set the parameters for the biped to walk successfully over the sloped terrain.  In this
preliminary study, since we would like to keep modifications to the level walking algorithm to a
minimum, we decide to keep the desired horizontal velocity unchanged and the torso at the same upright
posture while the biped walks on the sloped terrain.  We also decide to fix the desired step length of the
biped along the ground surface regardless of whether it is walking on sloped or level ground.  We change
only the desired hip height of the biped.  We use the global slope gradient to modify the desired hip height
for walking as described in the next paragraph.

          As in the case of level ground walking, the height limit of the biped for upslope is computed based on
the desired step length, the distance from the front ankle at which the double support phase transits to the
single support phase, and the singularity consideration of the back supporting leg during the double
support phase (see Figure 20 ).  Let´s denote h
li mi t
 to be the hip height limit measured vertically from a
global slope.  By geometric consideration, the hip height limit h
limit
 is computed by Equation (5.1).

                          h l l r r

                              limit
                                          = + - -

                                                    ( ) tan

                                                        1 2

                                                                           2 2 b

(5.1)

          where

                          r s l

                                        l t
                               = +

                                            cos b (5.2)

          Similar to level walking, a factor k

                                                                                                               hei ght
 is multiplied to the height limit h
li mi t
 to calculate the desired
height of the hip from a global slope.  The desired hip height z
d
 defined in Section 3.3.3  is then given by

Equation (5.3).

                                                                                        z k h x

                                                                                           d height limit
                                                                                                 = + tan b (5.3)

                                                                        where x  is the x-coordinate of the hip with respect to the stance leg´s ankle.

b

l

1
+l

2
r

h
limit

Transition plane
hip

                                                                                                                  Figure 20 .  Geometric constraint to calculate h
limit
: Level and upslope

                                                                        For the case of a downslope, both the back supporting leg during the double support phase and the

                                                              swing leg during the single support phase may reach singular configuration as shown in Figure 21 (a) and

                                                              Figure 21 (b), respectively.  For the latter case, we assume that the vertical projection of the hip is half way

                                                              between the front and back supporting legs when the swing leg touches down (see Subsection 3.3.2 ).

                                                              Thus, the height limit h
limit
 is computed as in Equation (5.4).

                                                                                        h l l r r

                                                                                           limit
                                                                                                        = + - +

                                                                                                                  ( ) tan

                                                                                                                      1 2

2

1

2

1
b (5.4)

                                                                        where

                                                                                        r s

                                                                                                               l

                                                                                          1
                                                                                                     0 5
                                                                                               = . cos b (5.5)

                                                                        The minimum of the computed hip height limit h
li mi t
 between Equations (5.1) and (5.4) is used to

                                                              compute the desired hip height z
d
 in Equation (5.3) during the downslope walking.  These equations can

                                                              also be used for level walking where b   is zero.  Note that the foot´s dimension is ignored in all

                                                              computations.

- b

l

1
+l

2
h
limit
r

stance leg
hip

transition plane
x

z

(a)

- b

l

1
+l

2

h
limit
r

1

0.5s

1

hip

swing leg
x

z

(b)

                                                                         Figure 21 .  Geometric constraint to calculate h
limit
 during downslope walking: (a) case 1; (b) case 2

                                                                        The strategy to control the swing leg control for both the upslope and the downslope walking is the

                                                              same as that for level ground walking.  The step length for the slope walking is measured along the slope

                                                              and the maximum lift height of the swing leg is measured perpendicular to the slope.

                                                              5 .1 .2 Transition  cases

                                                                        This subsection considers transitional walking from level ground to slope and slope to level ground,

                                                              where the slope can be either ascending or descending.  We first discuss the level-to-upslope and

                                                              downslope-to-level transition.

                                                                        For level-to-upslope transition, we employ a strategy similar to the one adopted by [Zheng and Shen,

                                                              1990].  In their approach, when their biped was walking statically from level ground to an upslope

                                                              surface, it employed a ^compliant~ stepping motion when the foot of its swing leg first came into contact
with the sloped surface.  The position and orientation of the landing foot were determined by the force
information generated by the force sensor underneath the foot at the moment of the contact.  The landing
foot could then comply with the constraints of the ground.  However, the bandwidth of such a strategy is
usually small.  Thus, it cannot be applied to the dynamic walking of our biped in which large bandwidth
control is desirable.

          At the moment when the swing foot touches the upslope surface, instead of using the force feedback
approach, we set the ankle torque of the swing leg to zero.  This allow the swing foot to orient itself and
adapt to the slope according to its natural compliance.  The whole process is shown in Figure 22 .  Before
the swing foot touches the slope surface, it is swung in the same manner as in level ground walking.

When the swing foot toe touches the slope surface (assuming the swing foot´s gradient with respect to the
level ground is zero initially), the state machine makes a transition from single support to single-to-double
transition phase and the ankle torque is set to zero.  A sufficiently small angle m  between the impact
force and the normal of the slope (see Figure 22 (a)) will result in an equivalent counter-clockwise moment
acting on the foot about the ankle (see Figure 22 (b)).  The counter-clockwise moment causes the foot to
rotate in a counter-clockwise direction until the heel touches down ( Figure 22 (c)).

          This strategy requires the ankle to be as low as possible (preferably below the foot) and m  to be small.

However, this may not be achievable, for example, m  is high if the friction coefficient of the slope surface
is high.  To enhance the strategy, we add a local PD position control at the ankle to prevent the impact
force from turning the foot in a clockwise direction.  The swing foot´s gradient can also be tilted so that
the toe is higher than the ankle.

                                                   Direction of swinging

                                      Ankle

                                                                          Impact force

                                                                   m

Direction of swinging

Ankle

Direction of swinging

Ankle

Equivalent moment
due to the impact
force

                                              (a) (b) (c)

                                                                                  Figure 22 .  Natural compliance of the swing foot

          When both the heel and the toe of the swing foot are on the slope, they trigger the transition from the
single-to-double transition phase to the double support phase.  The biped then computes the gradient of
the global slope based on the joints´ angles.  Note that the global slope gradient is not the same as the real
slope gradient since both feet are not on the same slope yet (see Figure 23 (a)).  The global slope is an
imaginary intermediate slope whose gradient is between the level ground gradient (equal to zero) and the
actual upslope gradient.  However, the biped considers the global slope to be the actual terrain slope
during the double support phase.  It computes the desired walking height based on the global slope.

          When the biped switches to single support phase, it continues to compute the desired walking height
based on the global slope.  The swing leg trajectory of the single support phase is also planned using the
global slope.  However, when the biped is at double support phase again, both its legs are on the actual
slope and the global slope will have the same gradient as the actual slope (see Figure 23 (b)).

          Note that during transition walking, the actual step length of the biped may vary significantly from the
desired step length.  For the level-to-upslope transition, the variation in the step length is due to the
premature landing of the swing foot.  The biped will reach a steady walking gait as it continues to walk on
the same slope.  The strategy for the level-to-upslope transition is also applied to the downslope-to-level
transition.

          In the computation of the desired hip height of the biped, an alternative strategy is to use the local
slope gradient instead of the global slope gradient.  However, this approach is not good in certain extreme
cases.  One example is when the biped steps onto a local variation in a terrain (see Figure 24 ).  In this
case, if the biped were to use the local slope gradient to compute its desired hip height, the hip would
follow trajectory (1) which is steep.  That is, the biped may ^amplify~ the terrain unnecessarily.  A drastic
action would result even though the actual terrain may not be rough.  However, if the intermediate global
slope gradient is used, the biped will go along trajectory (2) which is less steep compared to trajectory (1).

The usage of the intermediate global slope gradient will allow the biped to have a smoother transition than
if it were using the local slope gradient.

Global slope

Trajectory of
swing leg

Trajectory of
swing leg

(a)

(b)

                                                                Figure 23 .  (a)  Global slope whose gradient is different from that of the actual slope; and (b) global slope
whose gradient is the same as that of the actual slope.

Local slope

Trajectory (1)

Trajectory (2)

                                                                Figure 24 .  Extreme example to demonstrate a potential problem when the local slope is used to calculate
the desired hip height.

                                                                        This paragraph looks at the level-to-downslope and upslope-to-level transitions.  During the level-to-

                                                              downslope transition, the biped executes the usual walking control for single support phase until the

                                                              swing time has expired.  When the swing time has expired, if the swing foot has not touched down, the

                                                              biped will exert a preset downwards force exerted at the swing leg´s ankle so that the swing foot will

                                                              continue on its way down.  The downwards force will cause the swing leg´s ankle to penetrate through a

                                                              virtual surface (which is the global slope) (see Figure 25 (a)).  When the virtual surface is penetrated, the

                                                              biped re-computes the gradient of the global slope based on the instantaneous position of the swing leg´s

                                                              ankle (see Figure 25 (b)) and adjusts the desired hip height accordingly.  This is a continuous process.

                                                              After the swing leg has touched down 11 , the state machine will switch to the double support state and the

                                                              biped will compute the intermediate global slope (see Figure 25 (c)).  In this state, the biped will compute

                                                              11  When both heel and toe´s sensors are turned on.

                                                              the desired hip height based on the global slope.  The swing leg of the next single support state will also

                                                              follow this global slope.  The biped then goes through the whole sequence ( Figure 25 ) again before both

                                                              feet are on the same slope.  The strategy for the level-to-downslope transition can also be applied to the

                                                              upslope-to-level transition.

(a) (b)

Global slope

Trajectory of
swing leg

Global slope

(c)

Figure 25 .  Sequence for level-to-downslope transition

                                                                        For both the level-to-downslope and upslope-to-level transitions, we have to control the swing leg so

                                                              that it will not hit the ground prematurely (see swing leg trajectory (1) of Figure 26 ).  To avoid such an

                                                              event, the desired lift height for the swing leg should be set to a value which will enable it to clear all the

                                                              edges of the level-to-downslope and upslope-to-level transitions.  This is based on the assumption that we

                                                              know the maximum change in the gradients for each slope transition.

Trajectory of
swing leg

Global slope

Trajectory of
hip

(2)

(1)

Figure 26 .  Possible problem with swing leg

                                                                        For the level-to-downslope and upslope-to-level transitions, the swing leg may land on the edge

                                                              formed by the intersection of two different slopes.  This problem can be solved by several approaches, for

                                                              example, by adding more sensors to the feet and adding more event checks in the algorithm; by designing

                                                              a foot which can accommodate the edge, etc..  This problem will not be studied in this thesis.  We assume

                                                              that all the slope transitions are smooth.

                                                              5 .2 Extension to dynamic stair-walking

                                                                        The strategies developed for the biped to walk blindly over sloped terrain can be extended to dynamic

                                                              stair-walking.  However, in stair-walking, the biped requires prior knowledge of the stair profile.  This is

                                                              similar to a human who needs to rely on visual capability so that he knows the general location and layout

                                                              of a flight of stairs before he can walk dynamically on it.  The swing leg trajectory needs to be more

                                                              precise than that for sloped terrain walking since stairs usually have limited foothold area.  In our

                                                              analysis, we assume that the biped can always find a foothold on the stairs.

                                                                        The concept of global slope is also used in stair-walking ( Figure 27 ).  For stair-walking, at the start of

                                                              the single support phase, the biped will compute a global slope which joins the target ankle position of the

                                                              swing leg (when the swing foot lands on the desired foothold position) and the stance leg´s ankle.  This is

                                                              different from the sloped terrain walking in which the global slope is computed at the beginning of each

                                                              double support phase.

Global slope

Desired
trajectory of
swing leg

(a)

(b)

Desired
trajectory of
swing leg

Figure 27 .  Global slope in stair-walking

C h a p t e r

6 Simulations results

          This chapter first describes two sloped terrain profiles that were used in the simulation.  The
simulations´ parameters and results of the biped walking on these terrains are also included.  The purpose
of the simulations was to validate that the strategy developed in the previous chapter could be used to
achieve blind  walking over sloped terrain.  The sloped terrain was assumed to have a maximum absolute
gradient of 20 o .

          The robustness of the sloped terrain strategy was also illustrated by simulating the biped walking over
a series of random slopes.  We had also replaced the vertical virtual component (the one which used a
spring-damper) by Robust Adaptive Controller (Chapter 4 ) and let the biped walk over the same terrain.

          In all the simulations, we had assumed no slippage of the biped´s feet when they were in contact with
the ground and the terrain transition was smooth.  We assumed that the feet had shock absorbing material
to reduce the effect of impulsive force when it hit the terrain prematurely.  We had also assumed perfect
actuators at all the joints.  Note that the biped did not have any prior information of the terrain´s profile.

Therefore, it had to  feel  its way through the terrain based on the simple discrete (on/off) sensors at the feet
and the joints´ position sensors.

6 .1 Sloped terrain profiles used in the simulations

          This section describes two profiles of sloped terrain used in the simulation.  In both profiles, we
limited the gradient change at terrain transitions to 20 o .  And we only allow at most one terrain transition
per step.  The maximum absolute gradient at any point of the terrain was 20 o .

          We defined sloped terrain profile one  to be one which consisted of the following sequence of
transitions: level-to-upslope, upslope-to-level, level-to-downslope, downslope-to-level, where the upslope
and the downslope had gradients of 20 o  and -20 o , respectively.  The profile of this terrain is shown in the
top graph of Figure 29 .  This terrain was used in the simulation so that we could observe and compare the
key output variables for the upslope, downslope and transition terrain walking of the biped.

          The sloped terrain profile two  (see the top graph of Figure 31 ) was rougher than profile one .  The
sloped terrain profile two  was used to illustrate the robustness of our approach for the biped to walk over a
sloped terrain which consisted of a series of unknown slopes.  We had also simulated the biped walking on
this sloped terrain profile using Robust Adaptive Controller (Chapter 4 ).

6 .2 Walking over the sloped terrain profile one

          The purpose of this simulation was to study the walking pattern for upslope, downslope and transitions
based on the strategy developed in Chapter 5 .  The desired values of some of the gaits´ variables and the
parameters of the virtual components were set as in Table 6 .  Note that the desired hip height of the biped
was computed by the algorithm based on the desired step length and the instantaneous global slope.  The
initial values of the variables were set to be equal to the desired values in the simulation.  Although the
desired hip height for level ground walking was computed to be about 0.76m, the initial hip height of the
biped was set to 0.68m in the simulation.

               Table 6 .  Desired values of some of the gaits´ variables and the parameters of the virtual components
set in the simulation

                             Variable/parameter Notation Value

                             Desired pitch angle of the torso a
d
0 rad

                             Desired horizontal velocity of the hip v
xd
0.4 m/s

                             Desired step length s
l
0.28 m

                             Distance from the front ankle at which double

                             support phase transits to single support phase

l
t
-0.03m

                             Desired lift height of swing leg h
l
0.07 m

                             Parameters of virtual components:

                             1. Spring stiffness (in z direction) k
z
1000 N/m

                             2. Damping coefficient (in z direction) b
z
200 Ns/m

                             3. Damping coefficient (in x direction) b
x
200 Ns/m

                             4. Spring stiffness (in a direction) k
a
50 Nm

                             5. Damping coefficient (in a direction) b
a
20 Nms

          Figure 28  shows a stick diagram of the biped walking over the sloped terrain profile one  from left to
right.  Figure 29  and Figure 30  show the profiles of the key variables and the joints´ torque, respectively.

In Figure 29 , the vertical ^dash-dot~ and ^dotted~ lines represent the start of the single support and the
double support phases, respectively.  In Figure 30 , the vertical ^dash-dot~, ^dotted~, ^dashed~,

^continuous~ lines represent the start of Right Support, Double Support 2, Left Support and Double

Support 1 states, respectively.

          The top second graph of Figure 29  shows the discrete changes in the global slope gradient when the
biped walked over the terrain.  The actual upslope and downslope gradients were +0.35 rad (20 o ) and -

0.35 rad, respectively.  We could observe that at each of the transition locations (at x m
» 0 8 4 7 6 10

. , . , ,

   ),
there was at least one intermediate global slope which had a gradient between the level ground and the
actual slope gradient.  This helped to provide a ^smooth~ transition when the biped walked over these
transition locations.

          The top third graph of Figure 29  shows the actual hip height profile (solid line) of the biped measured
from the global slope.  This result shows that the biped was able to track the desired hip height (dashed
line) within a tolerable range.  The ripple found in the actual hip height profile was mainly due to the
swing leg dynamics and the variation in the effective mass of the biped as perceived at the hip.

          We observe that when the global slope gradient was negative, the desired hip height 12  (dashed line in
the top third graph of Figure 29 ) of the biped was higher than when the global slope gradient was positive.

This was the result of the geometric considerations (subsection 5.1.1 ) when we computed the desired hip
height of the biped.

          For the level-to-upslope transition, a substantial lowering of the desired hip height (from 0.76 m to

0.68m, see Figure 29 ) helped in the transition because the dynamic tendency of the biped at the moment
before its swing foot hit the upslope was to travel horizontally.  This lowering of the desired hip height
helped to prevent drastic changes in the vertical virtual force F
z
 required to divert the biped to walking
along the upslope.  We can observe in the same graph that the transitional variation in the actual hip
height (between x  = 0.5 m and 1.5 m) during this transition was quite smooth.

          For the upslope-to-level transition, the change from low to high (from 0.68 m to 0.76 m) in the desired
hip height of the biped relative to the global slope also helped to smooth the transition.  This could be
explained by the same dynamic behavior as in the previous paragraph.  The transitional variation in the
actual hip height of the biped (between x = 4.5 m and 5.5 m) was also observed to be smooth.

          For level-to-downslope transition, we observed that the variation in the desired hip height (around x  =

6.2 m) was not very large.  However, the variation in the vertical virtual force F
z
 was very large.  This
might have been due to the discontinuous change in the desired hip´s trajectory.

          For downslope-to-level transition, the variation in the vertical virtual force F
z
 was not so large.  The
impact of the swing leg when it hit the level ground could have provided an impulse which happened to
assist in the discontinuous change of the desired hip´s trajectory.

12  Relative to the global slope.

                                                      From the horizontal velocity profile of the hip (

�x  vs x ) in Figure 29 , we observed that the velocity

fluctuation was higher for the upslope walking than for the downslope walking.  This was mainly due to

two causes.  First, the dynamic frequency of the biped during the single support phase 13  was higher for the

upslope walking than for the downslope walking.  This is because the hip height of the biped (measured

from the slope) was lower in the former.  Thus, for the upslope walking, the horizontal velocity of the hip

increases at a rate relatively faster after the vertical projection of the biped´s center of gravity crossed over

its stance ankle during the single support phase.

          The swing leg trajectory was the second cause for the difference in the velocity profile.  We observed

from the stick diagram that the swing leg had different trajectories for the upslope, downslope and level

walking.  Hence, the dynamic disturbance of the swing leg for each of the cases were also different.  This

resulted in different velocity profiles for the three cases.  For example, in the upslope walking, the swing

leg started from a configuration which was closer to the singular configuration (ie., fully straightened),

thus causing higher disturbance to the horizontal velocity.

          The horizontal velocity also deviated significantly from the desired value at the upslope-to-level

transition and the level-to-downslope transition.  This was mainly due to the fact that the biped took

additional time to feel  the ground at these locations during the single support phase.  This delay in step

time resulted in slightly higher horizontal velocity when the biped reached the next double support phase.

We also observed the horizontal hip velocity, just after the touch down of the swing leg, was a fraction of

the velocity just before the touch down.  This was due to the impact effect of the swing leg when it touched

down [Kajita and Tani, 1991].

           Figure 28 .  Stick diagram of the biped walking over the sloped terrain profile one  from left to right

                                                          (spaced approximately 0.08 s apart and showing only the left leg)

13
     Similar to an inverted pendulum.

Figure 29 .  Profiles of the key variables when the biped walked over the sloped terrain profile one

Figure 30 . Torque profiles of the hip and the knee joints when the biped walked over the sloped terrain

profile one

6 .3 Walking over the sloped terrain profile two

          The purpose of this terrain profile was to demonstrate the robustness of the strategy developed for

sloped terrain walking.  The desired values of some of the gait variables and the parameters of the virtual

components were set as in shown Table 6 .  The initial values of the variables were set to be equal to the

desired values in the simulation.  The initial hip height was set to 0.64m and this is the same as the

desired hip height for walking on level ground.  Figure 31  shows the profiles of the key variables.  The

vertical ^dash-dot~ and ^dotted~ lines represent the start of the single support and double support phases,

respectively.

          Note that the profile of the terrain was not known to the biped in advance.  The biped was required to

feel  its way through the terrain.  From Figure 31 , we observed that the biped could cope with this rougher

terrain without much difficulty.  The actual hip height, hip horizontal velocity and pitch angle of the torso

were well-behaved in the simulation.

          Based on the analysis in Chapter 4 , we replaced the vertical virtual spring-damper with Robust

Adaptive Controller.  The following parameters: l  = 2, k=100, g =10, D=5, �m
o

=9, were used for Robust

Adaptive Controller; the other parameters and the desired values of the gaits´ variables were the same as

those listed in Table 6  except for l
                                                                                                   t

                                                                                                     (the distance  from the front ankle at which the double support phase

transits to the single support phase) which was set to 0.03m.  The initial values of the pitch angle of the

torso and the horizontal hip velocity were set to be equal to the desired values in the simulation.  The hip

height was set to 0.7m initially.  The biped was assumed to start from Double Support 1 state.

          The simulation result of the biped walking on sloped terrain profile two  is shown in Figure 32 .  It

showed that the biped walking using Robust Adaptive Controller was comparable with the previous

implementation which used only springs and dampers.  However, compared to the previous

implementation where the average horizontal velocity of the hip was generally lower than the desired

value, this implementation had higher velocity than the desired value.  This was mainly due to the fact

that we had set l
                                                   t

                                                     (the distance  from the front ankle at which double support phase transits to single

support phase) to a new value (0.03m) in this implementation instead of previous value (-0.03m).

          We observed that the estimated mass �m  did not converge to a constant value.  It was because at the

beginning of most of the double support phases, the actual hip heights of the biped deviated slightly and

randomly from the desired hip heights.  The randomness of the deviations was due to the randomness of

the terrain.  Robust Adaptive Controller was not configured to identify or ignore such error signals.

Hence it tried to adapt to them.  As long as the parameters of Robust Adaptive Controller were properly
selected, for example, choosing a high value for the bound f , the overall performance of such

implementation should still be robust.

                   Figure 31 . Profiles of the key variables when the biped walked over sloped terrain profile two

Figure 32 . Variables´ profiles of the biped walking over the sloped terrain profile two  using Robust

           Adaptive Controller as the vertical virtual component ( l  = 2, k =100, g =10, D =5, �m
o

=9)

6 .4 Walking on stairs

          In this section, the simulation results of a stair-walking are included.  The selected stair profile is

shown in the first graph of Figure 34 .  Each step of the stairs was 0.1m in vertical variation and 0.25m in

horizontal width.  The biped was assumed to know the profile of the stairs in advance.  The desired

variables and the parameters were set as shown in Table 6  except for the desired horizontal velocity of the

hip and the lift height.  The desired horizontal velocity of the hip was reduced to 0.2m/s since the slope of

the stairs was quite steep.  The lift height h
l

 was set to 0.1m for level ground walking and 0.2m for stair-

walking.  In the simulation, the initial value of the pitch angle of the torso and the horizontal velocity of

the hip were set to the desired values.  The initial hip height was set to 0.74m.  The biped was assumed to

start from Double Support 1 state.

          Figure 33  shows the stick diagram (only the left leg is shown) of the biped walking over the stairs from

left to right.  Figure 34  shows the profiles of the key variables.  The vertical ^dash-dot~ and ^dotted~ lines

in Figure 34  represent the start of single and double support phases, respectively.  The key output

variables were well-behaved and thus validated the applicability of the global slope  concept to stair-

walking.  Note that there was no intermediate global slope which existed in sloped terrain walking.  We

could have also incorporated in stair-walking some intermediate global slopes at the transition locations to

smoothen the transitions.

            Figure 33 .  Stick diagram of the biped walking on the stairs (spaced approximately 0.2 s apart and

                                                                                                                  showing only the left leg)

Figure 34 . Output variables profiles of the biped walking over the stairs

6 .5 Discussion

          This chapter has demonstrated by simulation that a planar biped is capable of walking blindly over a

two-dimensional random sloped terrain using virtual spring and damper components.  The notion of

global slope  was used to plan the desired trajectory of the biped´s hip.  The natural compliance of the

swing foot was also used for the swing foot to orientate itself along the local slope  during touch down.  As

long as the maximum absolute gradient of the sloped terrain and the maximum transitional change in the

gradient are below certain limits, the strategy developed for the sloped terrain walking can result in stable

walking.

          To apply the level walking algorithm for sloped terrain walking, we modified the algorithm based on

the geometry.  Given a desired step length, we let the biped walk with the body as high as possible without

causing the legs to reach singular configurations.  This resulted in a desired body height which varied

with the slope gradient.  This is different from [Kajita and Tani, 1991] approach in which the body height

of the biped was fixed regardless of the slope gradient.

          Virtual Model Control (VMC) approach results in a motion similar to the Linear Inverted Pendulum

mode described in [Kajita and Tani, 1995].  In the latter, a linear trajectory (or constraint line) was

formed based on the projected foothold position of the swing leg.  A simple dynamic equation based on a

massless leg model of the biped was used to obtain the dynamics of the biped travelling along the

constraint line.  However, to realise the constraint control, Kajita and Tani used inverse kinematics and

applied local position feedback at the joints.  In the VMC, we do not need to solve any inverse kinematics

and inverse dynamics of the biped [Pratt, 1995].  We simply let the virtual components generate the

required cartesian forces.  These forces are then transformed by a matrix to the joints´ torque.  If the biped

had massless legs, the VMC using the virtual components described in Section 3.3  would also generate a

linear trajectory in cartesian space.  In the VMC, the resulting equations for controlling the biped are even

simpler than those used in [Kajita and Tani, 1995] but we need to use some intuition in the former case.

Nonetheless, both approaches have shown that we do not need to have a complex control algorithm in

order to control a biped to walk dynamically on level or sloped ground.

          In the VMC, the biped behaves as if there is a passive suspension between the ground and the biped´s

body.  For sloped terrain which we assume to have no vertical step variation along its path, it is not

required to have active suspension 14  described by [Raibert, 1986a].  The biped simply tries to swing the

leg to achieve a desired step length, but if the swing leg prematurely hits a slope surface, the actual step

14
     [ Raibert, 1986a] used this term to explain the advantage of a legged machine that it could choose a foothold

      location so that the body would be decoupled from the unevenness of the terrain.

length will be shorter than the desired value.  When this happens, the biped will go to the next single

support phase earlier.  This is just how a human will react when he walks up a ramp from a level surface

blind-folded.  Hence, for the sloped terrain, we do not need to know the terrain profile in advance.

However, for stair-walking, the active suspension approach is required since the biped cannot place its

swing foot arbitrarily on the terrain.  This is the same for humans.  We will not be able to walk

dynamically on stairs without knowing their general location, layout, and approximate size.  However,

humans are much more advanced in that we do not need to know the exact  dimensions of the stairs to

walk steadily over them.

          There are still a number of future areas to be addressed.  One of which is the effect of the swing leg

dynamics and its disturbance on the body during the single support phase.  It will also be interesting to

compare various walking postures and their effects.  For example, we might want to change the bending

direction of the legs and study its effect on sloped terrain walking.

          We are also looking at the usage of the ankle torque to assist the walking.  For example, it can be used

to control the horizontal velocity to a limited extent [Kajita and Tani, 1995].  Besides using the ankle,

there are also a few other means of controlling the horizontal velocity.  We should try to find out which of

them are effective and under which conditions they are effective.

          We need to study the effect of changing other gait parameters like the torso pitch, desired horizontal

velocity, double to single support transition distance, step length, etc., on the stability of slope walking.

However, we will first need to define a performance index for rough terrain walking.

          We had assumed in the simulations that there was no slippage problem.  In real application, we

foresee a good foot design and a good swing leg control will be necessary so that slippage will not occur in

the real implementation.

          Although the study was limited to a planar biped, the information obtained would still be useful for 3-

D walking since the dominant walking dynamics of a biped happens in the sagittal plane [Raibert, 1986a].

If we can decouple partially or completely the frontal plane motion from the sagittal plane motion, we

should be able to use the algorithm developed in this thesis for 3-D walking bipeds.

          The VMC approach may not be the best and definitely not the only approach, but it is very simple to

implement.  Most importantly, most of the parameters and variables of the VMC approach possess some

intuitive sense.  This has compensated for the weakness of the VMC that it does not utilise the dynamic

equations of the system for control.  However, its present approach (using spring-damper as the virtual

components) may not be applicable to transient motion control which generally requires either dynamic or

energy information of the system.

C h a p t e r

7 C onclusions  and  Further Work

7 .1 Conclusions

          This thesis has demonstrated the successful simulation of the application of Virtual Model Control

(VMC) to a seven-link planar biped for it to walk dynamically  and steadily  over sloped terrain with

unknown slope gradients and transition locations.  It assumed that the slope gradients were between -20 o

and +20 o ; and the sloped terrain had maximum transitional gradient change of less than 20 o .  The

developed algorithm for sloped terrain walking was based on the level ground implementation and only

minor changes were needed.  In the implementation, a virtual surface  was defined using a global slope

computed at the beginning of each double support phase.  The algorithm then computed the desired hip

height based on the global slope and resulted in a straight line trajectory parallel to the virtual surface.  It

was very simple to implement and did not require an extensive sensory system to achieve blind walking.

The main knowledge required for the implementation was intuition and geometric considerations.  The

plausibility of the VMC approach to control the biped to walk steadily and dynamically over unknown

sloped terrain without any dynamics computation may seem too good to be true.  This coincides with a

statement made by M. Raibert [Raibert, 1990]: ^ A legged system can exhibit complicated dynamic

behavior without requiring a very complicated control system .~

          We have also replaced the vertical virtual spring-damper with Robust Adaptive Controller which was

successfully implemented for the biped to walk over random sloped  terrain.  This thesis has also shown

how the algorithm for sloped terrain walking can be modified so that it can be used for the stair climbing

task.

7 .2 Further Work

          To refine the algorithm further, we will formulate a performance index for sloped terrain walking.

Based on such an index, we can then implement some optimization or learning control techniques for the

biped to select a good set of variables for robust sloped terrain walking.

          We will also apply the algorithm developed in this thesis to 3-D walking.  To achieve this, we will

need to design a 3-D biped whose frontal plane motion control can be decoupled partially or completely

from the sagittal plane motion.

Appendix  A:

Equations to convert virtual forces to joints´ torque

          A.1  Double Support Phase

          The equations to convert virtual forces to joints´ torque during the double support phase was derived in

[Pratt, 1995] as shown in Equation A.1.  Note that the subscript l  denotes the left leg and r  denotes the

right leg and the sign convention is shown in Figure A.1:

                             t

                             t

                             t

                             t
a

                                 lk

                                 lh

                                rk

                                 rh
x

z

                                                       CV

                                                          E

                                                                                DV

                                                                                   E

                                                                                                      V QD RC

E

                                                          AW

                                                             E

                                                                                   BW

                                                                                      E

                                                                                                          W SB TA

E

F

F

M

                          é

                          ë

                          ê

                          ê

                          ê

                          ê

                                      ù

                                      û

                                      ú

                                      ú

                                      ú

                                      ú

                                          =

                                                                                                             + -
+

+

                                                    - -

                                                                                                     - - +
+

                                                 é

                                                 ë

                                                 ê

                                                 ê

                                                 ê

                                                 ê

                                                 ê

                                                 ê

                                                 ê

                                                 ê
ù

û
ú

ú

ú

ú

ú

ú

ú

ú
é

ë
ê

ê

ê
ù

û
ú

ú

ú

                                                                                                                     2

1

2

                                                           0 0

1

2

                                                                                                                     2

1

2

                                                           0 0

1

2

(A.1)

where

                                                    A L L
                                                                                         la la lk

                                                          = - - +
                                                                        1 2

                                                                           cos cos( )

                                                                                     q q q

                                                    B L L
                                                                                        la la lk

                                                          = - - +
                                                                        1 2

                                                                           sin sin( )

                                                                                    q q q

                                                   C L L
                                                                                        ra ra rk

                                                          = - - +
                                                                        1 2

                                                                           cos cos( )

                                                                                     q q q

                                                    D L L
                                                                                        ra ra rk

                                                           = - - +
                                                                        1 2

                                                                            sin cos( )

                                                                                     q q q

                                                    E CB AD

                                                          = -

                                                   Q L
                                                                                           la lk

                                                          = - +
                                                                        2

                                                                            cos( )

                                                                                        q q

                                                    R L
                                                                                          la lk

                                                          = - +
                                                                        2

                                                                            sin( )

                                                                                      q q

                                                   S L
                                                                                          ra rk

                                                         = - +
                                                                       2

                                                                           cos( )

                                                                                      q q

                                                   T L
                                                                                         ra rk

                                                         = - +
                                                                       2

                                                                            sin( )

                                                                                      q q

                                                  V QB RA

                                                          = -

                                                   W SD TC

                                                           = -

          A.2  Single support phase

          In the single support phase, due to the limp joint at the ankle, one of the virtual forces due to the

virtual components cannot be implemented.  In the actual implementation, we only adopt the vertical and

torsional motion control. The relation between the virtual force vector and the torque vector is shown by

Equation (A.2) [Pratt, 1995]:

                              0 1

1

                                                                                0 0 1

                                                      1 2 1 2

                                                                     2 2

                            t

                            t

                                                                  q q q q q q

                                                                                  q q q q

a

                                k

                                h

                                                                     a a k a a k

                                                                                     a k a k
x

z

                                                    L L L L

                                                                 L L

F

F

M

                          é

                          ë

                          ê
                          ê
                          ê

                                   ù

                                   û

                                   ú
                                   ú
                                   ú

                                      =

                                              - - + - - +

                                                            - + - +

                                            é

                                            ë

                                            ê
                                            ê
                                            ê
ù

û
ú
ú
ú
é

ë
ê
ê
ê
ù

û
ú
ú
ú

                                                          cos cos( ) sin sin( )

                                                                        cos( ) sin( )

(A.2)

          We simply allow the vertical virtual force F
z

 and the rotational virtual force M
a
to influence the

horizontal motion.  The first row of Equation (A.2) generates Equation (A.3) which shows the equivalent

                                                              horizontal virtual force on the biped´s hip if the vertical virtual force F
z

 and the rotational virtual force

                                                                M
                                                                      a

                                                                            were to be implemented in the single support phase.

[ ]

                                                                                        F
                                                                                                              L L

L L

F

M

                                                                                            x
a a k
a a k
z
                                                                                                 = -
+ +

+ + -
é

ë
ê
ù

û
ú

1
1

                                                                                                                 1 2

1 2
                                                                                                                    cos cos( )
sin sin( )
q q q
q q q

a

(A.3)

                                                                        The Equation (A.4) [Pratt, 1995] was used to compute the hip and knee joints´ torque in the single

                                                              support phase.

                                                                                           t

                                                                                           t
q

q q q
q

q q q

a

                                                                                              k

                                                                                              h
k

a a k
a

a a k
z

L L

                                                                                                                L L

L

L L

F

M

                                                                                        é

                                                                                        ë

                                                                                        ê

                                                                                                  ù

                                                                                                  û

                                                                                                  ú

                                                                                                      =

-

+ + + +

                                                                                                            é

                                                                                                            ë

                                                                                                            ê

                                                                                                            ê
ù

û
ú

ú
é

ë
ê
ù

û
ú

1 2

                                                                                                                    1 2

1

1 2
0 1
sin

                                                                                                                       cos cos( )
cos( )

cos cos( ) (A.4)

z

x
l
1
l2

- q

k

q

a

A

B
z

q

h

z
t

h

t

k

t

a

Figure A.1.  The notations and sign convention

                                                      Appendix  B:

                                                      Stability analysis based on ^massless legs~ model

                                                                This appendix analyzes the stability of Virtual Model Control (VMC) application (as described in

                                                      Section 3.3 ) to steady dynamic walking of the biped.  Since the masses of the biped´s legs are small

                                                      compared to the body mass, we reduce the model to one which has massless legs as shown in Figure B.1.

                                                      We have also ignored the transition phases because they are very similar to the single support phases.  Let

                                                       [ , , ]

                                                          x z

                                                                             T
                                                                     a be the generalized coordinates which locate the cartesian frame ox
b
z
b

 attached to the body with

                                                      respect to the inertia cartesian frame OXZ, [ , , ]

F F M
x z

T
a

 be the generalized forces and  [ , , ]
d d d
x z

T
a

 be

                                                      the disturbances (e.g. due to the impact during the touch down of the swing leg) along each of the

                                                      generalized coordinates.  Also, let the body mass and moment of inertia (about the center of mass) be m

                                                      and I , respectively.  The center of mass of the body is at distance l  from the hip.  The resultant dynamic

                                                      equations of motion are simply

                                                                                 m x F d
                                                                                                     x x

                                                                                      � � = + (B.1)

                                                                                 m z F mg d
                                                                                                     z z

                                                                                     � = - + (B.2)

                                                                                 I M F l F l d

                                                                                                 M ml x m z mg l d

                                                                                                                       x z

                                                                                     � cos sin

cos � ( � � ) sin

                                                                                   a a a

a a

                                                                                                       a a

                                                                                                       a a

                                                                                          = + + +

                                                                                          = + + + +

(B.3)

                                                                In matrix form, they can be represented as follows

                                                                                      F

                                                                                      F

                                                                                    M

                                                                                                                       m

m

                                                                                                                 ml ml I
x

z mg

mgl
d

d

d

                                                                                         x

                                                                                          z
x

z

                                                                                          a a
a a a a

                                                                                 é

                                                                                 ë

                                                                                 ê

                                                                                 ê

                                                                                 ê

                                                                                               ù

                                                                                               û

                                                                                               ú

                                                                                               ú

                                                                                               ú

                                                                                                   =

                                                                                                            - -

                                                                                                         é

                                                                                                         ë

                                                                                                         ê

                                                                                                         ê

                                                                                                         ê
ù

û
ú

ú

ú
é

ë
ê

ê

ê
ù

û
ú

ú

ú

+

-
é

ë
ê

ê

ê
ù

û
ú

ú

ú

+
é

ë
ê

ê

ê
ù

û
ú

ú

ú

0 0

                                                                                                                       0 0

0

                                                                                                                        cos sin

� �

�

� sin

(B.4)

          The control laws based on the virtual components described in Section 3.3  are listed as follows

                           F b x x
                               x d

                                  : ( � � )

                                    = - (B.5)

                           F k z z b z z
                              z z d z d

                                 : ( ) ( � � )

                                    = - + - (B.6)

                           M k b
                                                             d d

                                 a a a

                                                        a a a a
                                     : ( ) ( � � )

                                        = - + - (B.7)

          where �x
                                  d

                                       , z
                                                d

                                                     and a
                                                                         d

                                                                               are the desired horizontal velocity of the hip, the desired hip height and the

desired body pitch angle, respectively.

          We can apply Modern Control theory to analyze the stability of such a system.  However, it is less

complex if we analyze the stability in each coordinate separately, especially for x  and z , where the

resulting closed loop equations are decoupled from other coordinates.

          For the vertical height control, we substitute Equation (B.6) into (B.5) and this gives

                          m z k z z b z z mg d
                                              z d z d z

                               � ( ) ( � � )

                                    = - + - - + (B.8)

          Without loss of generality, let´s neglect mg .  Rewriting Equation (B.8) in Laplace transformed form,

assuming zero initial conditions, we obtain

                          Z s

                                                         k b s

                                               ms b s k

                                                                                          Z s

                                                                                                                 ms b s k

D s

                                                            z z

                                                                     z z

                                                                                              d

z z
z

                               ( ) ( ) ( )

                                         =

                                                                 +

                                                            + +

                                                                                                           +

+ +

                                                       2 2

1
(B.9)

          Since m , b
                                        z

                                           and k
                                                           z

                                                              are strictly positive, this coordinate is stable (with closed loop poles lying in the left

half of the s-plane).  Also, the disturbance due to impact will be attenuated if its frequency is higher than

the bandwidth of the closed loop system along the z direction.

          For the horizontal velocity control, considering for the double support phase that the horizontal virtual

damper can be applied, we obtain the following equation by substituting Equation (B.5) into Equation

(B.1)

                          m x b x x d
                                              x d x

                               � ( � � )

                                    = - + (B.10)

          Since the input is velocity, we take the Laplace transform of Equation (B.10) (assuming zero initial

conditions) with respect to velocity v
                                                                                                       x

                                                                                                          and obtain the following

                          V s

                                                         b

                                                  ms b

                                                                        V s

                                                                                                  ms b

D s
                              x

                                                            x

                                                                   x

                                                                            xd

                                                                                                                    x
x

                                 ( ) ( ) ( )

                                           =

                                                           +

                                                                                            +

                                                                                                           +

                                                                                                           1
(B.11)

          Equation (B.11) shows that the horizontal velocity is stable and it converges to the desired velocity.

However, during the single support phase, we are not able to control this parameter.  Therefore, we can

only say that this parameter will not diverge if the double support phase is sufficiently long to correct the

error in velocity resulting from the single support phase.  We may also use other horizontal velocity

control methods, for example, by varying the foot placement of the swing leg.

          For the pitch angle control, we use the third dynamic equation (Equation (B.3)).  Note that the third

dynamic equation is nonlinear and there is coupling among the generalized coordinates: x, z and a .

However, since we are keeping the body upright throughout the walking cycle, we can linearize the
equation about a = 0 .  After substituting the control law (Equation (B.7)) into Equation (B.3) and

linearizing the resulting equation about a = 0 , the following equation is obtained

                           I k b F l d
                                                         d d x

                              � � ( ) ( � � )

                             a a a a a
                                             a a a

                                    = - + - + + (B.12)

          By taking the Laplace transform of Equation (B.12) (assuming zero initial conditions), we have

                           A s

                                                    k b s

                                             Is b s k

                                                                                   A s

                                                                                                                        l

                                                                                                       Is b s k

F s
l

Is b s k

D
                                                                                      d x

                              ( ) ( ) ( )

                                       =

                                                            +

                                                      + +

                                                                                                  +

                                                                                                                + +

+

+ +

                                                       a a

                                                             a a a a a a
a
                                                  2 2 2

   (B.13)

          Since I , b
                                      a

                                           and k
                                                            a

                                                                 are all strictly positive, the result shows that the control law for a  is locally stable.

Considering the double support phase where we can apply the virtual damper in the horizontal direction,

since the desired horizontal velocity is constant, F
x

® 0  after any transient motion.  This means that a

will approach a
                                             d

                                                  = 0 .  Even for the single support phase, we can choose a large value for k
a
to reject the

disturbance due to F
                                                         x

                                                             and d
                                                                                a

                                                                                      which we assume to be bounded.

          Note that, although the stability analysis done here assumes that the biped has massless legs, this does

not mean that the VMC cannot be applied to a biped which has significant leg masses compared to the

body.

                                                                                                             l
m,I

                                                                                                   z

x
z

b

x

b

- a

F

x

F

z

M

a

                                                                                                  o
o

b

                                                                                      Figure B.1.  Massless leg model for the biped

References

[Asada, 1986] H. Asada and J. E. Slotine, Robot Analysis and Control , Wiley, 1986.

[Furusho and Masubuchi, 1986]  J. Furusho and M. Masubuchi, ^ Control of a Dynamical Biped

       Locomotion System for Steady Walking ,~ Journal of Dynamical Systems, Measurement, and Control,

       Vol. 108, pp 111-118, June 1986.

[Kajita and Tani, 1996]  S. Kajita and K. Tani, ^Adaptive Gait Control of a Biped Robot based on

       Realtime Sensing of the Ground Profile,~  Proc. Of IEEE Internation Conference on Robotics and

       Automation , pp 570-577, April 1996.

[Kajita and Tani, 1995]  S. Kajita and K. Tani,  ^Experimental Study of Biped Dynamic Walking,~  Proc.

       of IEEE International Conference on Robotics and Automation , May 1995.

[Kajita and Tani, 1991]  S. Kajita and K. Tani, ^ Study of Dynamic Biped Locomotion on Rugged Terrain:

       Derivation and Application of the Linear Inverted Pendulum Mode ,~ Proceedings of the 1991 IEEE

       International Conf. on Robotics and Automation, California, pp 1405-1411, April 1991.

[McGeer, 1990]  T. McGeer, ^Passive Dynamic Walking,~ International Journal of Robotics Research ,

       vol. 9, no. 2, pp 62-82, 1990.

[Mitobe, et al., 1995]  K. Mitobe, N. Mori, K. Aida and Y. Nasu, ^Nonlinear Feedback Control of a Biped

       Walking Robot,~  Proc. of IEEE International Conference on Robotics and Automation , pp 2865-2870,

       1995.

[Muybridge, 1989]  E. Muybridge, The Human Figure in Motion.  Published by Dover Pubns, 1989.

[Pratt, 1995]  J. E. Pratt, ^Virtual Model Control of a Biped Walking Robot,~  Master Thesis for

       Department of Engineering in Electrical Engineering and Computer Science, MIT, August 1995.

[Pratt and Williamson, 1995]  G. A. Pratt and M. M. Williamson, ^Series Elastic Actuators,~ Proc. of

       IEEE International Conference on Intelligent Robots and Systems , pp 399-406, 1995.

[Raibert, 1986]  M. H. Raibert, Legged Robots That Balance.  Cambridge, MA: MIT Press, 1986.

[Raibert, 1986a]  M. H. Raibert, ^Legged Robots,~  Communications of the ACM , vol.29, no.6, June 1986.

[Raibert, 1990]  M. H. Raibert, ^Legged Robots,~  Artificial Intelligence at MIT Expanding Frontiers ,

       Edited by P. H. Winston, MIT Press, vol. 2, pp 149-179, 1990.

[Slotine and Coetsee, 1986]  J.-J. E. Slotine and J. A. Coetsee, ^Adaptive sliding controller synthesis for

       non-linear systems,~  Int. J. Control, vol. 43, no. 6, pp 1631-1651, 1986.

[Slotine and Li, 1991] J. E. Slotine and W. P. Li, Applied Nonlinear Control , Prentice Hall, 1991.

[Song and Waldron, 1989]  S. M. Song and K. J. Waldron, Machines That Walk, MIT Press, 1989.

[Tzafestas et al., 1996]  S. Tzafestas, M. Raibert and C. Tzafestas, ^Robust Sliding-mode Control Applied

       to a 5-link Biped Robot,~ Journal of Intelligent and Robotics Systems ,  15, pp 67-133, 1996.

[Yamaguchi, et al., 1996] J. Yamaguchi, N. Kinoshita, A. Takanishi and I. Kato, ^Development of a

       Dynamic Biped Walking System for Humanoid: Development of a Biped Walking Robot Adapting to

       the Humans´ Living Floor,~  Proc. of IEEE International conference on Robotics and Automation , pp

       232-239, 1996.

[Yang, 1994]  J. S. Yang, ^A Control Study of a Kneeless Biped Locomotion System,~  Journal of the

       Franklin Institute , vol. 331B, no. 2, pp 125-143, 1994.

[Zheng and Shen, 1990]  Y. F. Zheng and J. Shen, ^Gait Synthesis for the SD-2 Biped Robot to Sloping

       Surface,~  IEEE Transactions on Robotics and Automation , vol. 6, no. 1, pp 86-96, Feb 1990.